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1940 waterproof lamp
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Please keep the instruction manual properly
1. Remove the packing
For the correct and safe use of this product, please read the instructions carefully before installing and using this product. This instruction contains important installation and application information, and please strictly follow the operation steps in the instructions when installing and operating the product. At the same time, please keep this instruction properly.

The 1940 waterproof lamp is designed and produced in strict accordance with CE standards, and conforms to the international standard DMX512 signal protocol. It can be used for control alone or online. It has the characteristics of fast rotation, low noise and powerful functions, and is suitable for small and medium-sized concerts, theaters, studios, nightclubs and bars.

Please be careful to remove the package. After removing the package, check whether the product is damaged during transportation and check whether the following contents are complete.

1940 waterproof lamp----1 signal line----1                                       1940 waterproof lamp----1 signal line----1
Instruction manual----1 power cord----1                                                Instruction manual----1 power cord----1                  









































2. Safety instructions


 pay attention to ！
Please be careful before operating this product. This product is a high voltage product. If you touch the wire, you may be electrocuted!

This product is in perfect condition before leaving the factory. To maintain its integrity and ensure safe operation, users should follow the safety instructions and warnings provided in this manual. Important: Any damage caused by not following this manual is not covered under warranty[image: 图片2]. The supplier is not responsible for any issues arising from non-compliance with the manual. If the product has been exposed to extreme temperature fluctuations (such as after transportation), do not immediately connect it to power, as condensation from temperature changes can damage the product. Wait until the product has returned to normal operating temperature before using it.
This product can be used in the voltage range of 90-240V, which is for indoor use. Please ensure that the ground voltage is not higher than the range that the product can withstand!! The power plug must be plugged into a class I socket with good protection. The green or tea-colored conductor must be grounded.
Please check the power cord of this product regularly. Ensure that the power cord is not folded or damaged, and do not connect it to other wires! Pay special attention when connecting the power cord or related wires. Unplug the power cord before using this product or cleaning.
Before using the product, please familiarize yourself with the operation function of the product. Please do not let children or unprofessional personnel touch the product.
Please do not shake this product. Do not use brute force when installing or operating the product. Do not allow unprofessional personnel to operate the product. Most damage is caused by unprofessional operation.
The product is not equipped with relevant maintenance parts. The maintenance and repair of the product can only be carried out by professionals!
Please do not change this product without authorization, otherwise the product may be damaged, so the damage caused is not covered by the warranty. In addition, unprofessional operation may lead to short circuit, burns or electric shock, etc.




3. Operation instructions

--This product is a shaking dyeing beam lamp, used to create dyeing performance effects.
--If the product has been exposed to a large temperature difference (for example, after transportation), do not start the product immediately, because hot shrinkage will damage the product. Please wait until the equipment reaches normal room temperature before starting the product.
--Pay attention to shockproof. Avoid strong collision during installation.
--Please do not lift the entire product through the lamp head, because the mechanical damage of the equipment may be caused.
--When selecting the installation location, make sure that the product is not exposed to overheating, too wet or dusty places. Do not place any wires on the ground, otherwise you may be at risk of electric shock.
--Before installing the product, make sure that the installation point is safe
--Secure the product with a safety rope and check all screws for correct installation
--Please ensure that the lens is in good condition. When the lens is damaged or scratched, please replace the lens.
It is recommended that the product be operated by a technician familiar with the product. Non-technical personnel are prohibited from operating this equipment, because many losses are caused by non-professional operation.
--Please keep the packing materials properly in case of secondary transportation.
--Do not change the product without the guidance of the manufacturer or distributor.
--Any equipment failure caused by not operating the equipment according to the instructions is not covered by the warranty. And any accident caused by short circuit, injury, electric shock, ultraviolet light, bulb explosion and so on are not covered by the warranty.

4. Product hanging and installation

Note: For safety, please hang the product away from aisles, seating areas, or areas accessible to people
Before hanging this product, please ensure that the installation point can withstand 10 times the weight of this product.
The product must be installed with double protection devices, such as safety ropes.
When hanging, removing or repairing this product, do not stand under the installation point.
Please ensure that the product should be installed at least 0.5 meters away from flammable materials.
Please remember to use a safety rope as a safety guarantee in case of accidents when fastening the lock.































Hanging point: The top hanging requires the installation personnel to be experienced, including calculating the load requirements, using the installation materials, and periodically checking the safety status of the installation materials and products. If you lack this knowledge, please do not try to install by yourself. If the operation is not correct, it may lead to serious consequences such as personal injury.
Before the product is powered on, please be sure to complete all required hanging and installation steps.
Quick lock hanging: This product has a specially designed professional hanging part at the bottom, including quick lock hanging part and safety rope hanging point (please refer to the figure below).
When hanging the product on the truss, please remember to use the appropriate quick lock, fix it at the quick lock hanging position of the product, and hang it with M10 screws. For further safety, install the safety rope at the bottom of the product and fix it on the truss.
[image: ]
No matter which type of suspension you choose, please remember to use a safety rope. The bottom of the product is equipped with a special safety rope hanging point, please refer to the picture above, and please remember to use the special safety rope hanging point, do not install the safety rope on the handle position.




































5.DMX-512 linkage 

Please connect the male XLR connector of this product to the controller's signal output port, and the female XLR connector to the signal input port on the back panel of this product. You can connect multiple units in series, and the signal cable must be three-core, shielded, and equipped with XLR input and output connectors. Please refer to the following diagram.
[image: LCA028 DMX链接图]
[image: 3-pin Connetor]                          [image: ]

DMX-512 connections require a terminator (loop connection)
During the installation process, if the signal cable needs to be laid over a long distance or in a noisy environment, such as a karaoke bar, it is recommended to use a DMX terminal (loop connection). This helps prevent digital control signals from being muddied by electrical noise. The DMX terminal consists of a simple XLR connector with 2 or 3 pins and a 120-ohm resistor. Insert the terminal into the XLR output port of the last device, as shown in the figure below.
[image: ]

































6. Menu description
· Menu desktop
 temperature ：**℃
◆ Humidity: display the humidity of the board
◆**℃: Current temperature

 humidity ：**





001
DMX-512 pattern 




◆ Current address code





◆ Current operating mode



· Menu home screen
[image: ]










◆ Address: Click to enter the address code Settings
◆ Settings: Click to enter the system Settings
◆ Test: Click to enter manual mode
◆ Calibration: Click the input password to enter the system calibration mode
◆ Reset: Click to enter the system reset mode
◆ Information: Click to view system information

· Menu structure

	 primary menu 
	Sub-menu
	Three-level menu/parameters

	 address 
	001 - 512
	(Add or subtract one value)

	
	 running mode 
	DMX/self-walk 1/self-walk 1/sound control

	
	 channel pattern 
	21CH/23CH/35CH/78CH/92CH/97CH/99CH

	
	The level is reversed
	On/off

	
	Vertical reversal
	On/off

	
	Hall error correction
	On/off

	
	Light coupling error correction
	On/off

	
	Signal is maintained
	On/off

	
	Screen protection
	On/off

	
	The screen flips
	On/off/automatic

	
	Update synchronously
	On/off

	
	 language 
	 the Chinese language /EN

	
	Screen lock
	On/off

	
	Speed mode
	Fast / standard

	
	 factory data reset 
	 affirm 

	
	
	 cancel 

	 manual mode 
	Current channel mode channel
	0-255

	 system calibration 
	 enter password 
	Lamp calibration

	 system reset 
	The effect motor resets
	 affirm 

	
	Reset the scanning motor
	 affirm 

	
	All motors reset
	 affirm 

	 system info 
	Reset error message
	Display the reset error message

	
	DMX data monitoring
	Receive the channel value from the console

	
	 sensor information 
	Hall information

	
	
	X-ray coupling information

	
	
	Y optocoupler information

	
	Hardware version
	Display the hardware version

	
	 software release 
	Display the software version



· Automatic screen rotation function
The system can automatically rotate the screen according to the direction of gravity, without manual rotation. You can also turn off the automatic rotation function.

·  manual control 
This interface is used to control the current lamp.
Press "OK" to enter the editing state. Press "up" and "down" keys to change the channel value. Press "OK" again to save the modified value, exit the editing, press "exit" to not save the modified value, and directly exit the editing.

·  system calibration 
A password is set here to prevent non-professionals from misoperating. Press the "OK" key for password verification.
	 option 
	 explain 

	Initial position calibration
	After entering the sub-interface, you can adjust the reset position of the motor of X axis, Y axis, focusing and rotation to make up for the error in hardware installation. The adjustment range is 0~255, and 127 means no adjustment.

	 white balance 
	After entering the sub-interface, you can adjust the white balance of red, green, blue and white of the lamp and LED1-19. The adjustment range is 0~255, and 255 means no adjustment.

	 power 
	After entering the sub-interface, you can adjust the power of the lamp, and the adjustment range is 0~255.255 means no adjustment.

	MIC sensitivity 
	Voice control sensitivity calibration.

	Focus control
	Control the focusing stroke, the adjustment range is 0~255,255 is the maximum value, 0 means no adjustment.

	 change password 
	Change the password entered in the system calibration interface.



·  reset 
Press the "up" and "down" keys to switch the reset mode, press "OK" and directly reset.
	 option 
	 explain 

	The effect motor resets
	The effect disk is reset except for XY

	Reset the scanning motor
	Only the XY axis is reset

	All motors reset
	Light fixture reset



·  system info 

	 option 
	 explain 

	Reset error message
	If the red ERR indicator light is on, it indicates that the lamp operation is wrong. You can enter the sub-interface to view the details.

	DMX data monitoring
	Thus, the sub-interface is entered to display the channel value numerically for viewing.

	 sensor information 
	Monitor the status of various photoelectric switches, Hall sensors and other sensors on the lamp in real time.

	Hardware version number
	Lighting hardware information.

	Software version number
	Lighting software version.



7. Product features
Voltage: AC90-240v 50-60HZ
Rated power: 760W
Light source: 19 high brightness LED beads of 40 watts (four-in-one RGBW)
Beam Angle: 5-55°
Strobe: 1-25 times per second with a variety of strobe effects
Dimming: 0-100% linear dimming.
Channels: 7 built-in channel modes 21CH/23CH/35CH/78CH/92CH/97CH/99CH
Control: DMX512, self-walking, voice control, RDM.
Horizontal scan: 540 degrees +16 bit fine tuning,
Vertical scan: 250 degrees +16 bit fine tuning
Display: Chinese and English display             
Carton packing size (one and one): 62*39*51cm
Net weight 24kg, gross weight 26.7kg                
 characteristic ：
1. Each lamp can be controlled separately.
2. The unique honeycomb design of the lens can rotate infinitely to create a variety of dreamy effects.
3. The display can automatically rotate 180° to accommodate different installation angles.
4. It integrates multiple effects such as focusing, beam, staining and pattern into one.
5. The scanning position memory function can be automatically reset.
6. The system has the function of fan cooling and automatic temperature detection. When the temperature is too high, the system will automatically stop working to protect the lamp.

8. List of access points
	 channel 
	 function 
	DMX numeric value 
	 description 

	1
	1
	1
	 red 
	0-255
	Linear dimming from dark to light

	2
	2
	2
	Red tweaks
	0-255
	Red 16bit dimming

	3
	3
	3
	 green 
	0-255
	Linear dimming from dark to light

	4
	4
	4
	Green tweaks
	0-255
	Green 16bit dimming

	5
	5
	5
	 blue 
	0-255
	Linear dimming from dark to light

	6
	6
	6
	Blue fine-tuning
	0-255
	Blue 16bit dimming

	7
	7
	7
	 white 
	0-255
	Linear dimming from dark to light

	8
	8
	8
	White fine-tuning
	0-255
	White 16bit dimming

	9
	9
	9
	Color temperature adjustment
	0-255
	 8000K-2500K

	10
	10
	10
	Color macro
	0-255
	10-120 valid 

	11
	11
	11
	 stroboflash 
	0-255
	 stroboflash 

	12
	12
	12
	General dimming
	0-255
	Linear dimming from dark to light

	13
	13
	13
	General dimming fine tuning
	0-255
	Total dimming 16bit

	14
	14
	14
	X axle 
	0-255
	0-540 degrees

	15
	15
	15
	X-axis fine-tuning
	0-255
	16-bit adjustable

	16
	16
	16
	Y axle 
	0-255
	0-205 degrees

	17
	17
	17
	Y-axis fine-tuning
	0-255
	16-bit adjustable

	18
	18
	18
	 macro 
	0-255
	

	19
	19
	19
	 reset 
	0-25
	Reset and clear 0

	
	
	
	
	26-76
	The effect motor resets

	
	
	
	
	77-127
	XY motor reset

	
	
	
	
	128-255
	All motors reset

	20
	20
	20
	 amplify 
	0-255
	The Angle is adjusted linearly from small to large

	21
	21
	21
	 revolve 
	0-127
	0-60 degrees

	
	
	
	
	128-188
	Counterclockwise from fast to slow

	
	
	
	
	189-193
	 cease 

	
	
	
	
	194-255
	Clockwise from slow to fast

	
	22
	22
	LED1-R
	0-255
	LED1-Red dimming

	
	23
	23
	LED1-G
	0-255
	LED1-Green dimming

	
	24
	24
	LED1-B
	0-255
	LED1-Blue dimming

	
	
	25
	LED1-W
	0-255
	LED1-white dimming

	
	25
	26
	LED2-R
	0-255
	LED2-Red dimming

	
	26
	27
	LED2-G
	0-255
	LED2-Green dimming

	
	27
	28
	LED2-B
	0-255
	LED2-Blue dimming

	
	
	29
	LED2-W
	0-255
	LED2-white dimming

	
	28
	30
	LED3-R
	0-255
	LED3-Red dimming

	
	29
	31
	LED3-G
	0-255
	LED3-green dimming

	
	30
	32
	LED3-B
	0-255
	LED3-Blue dimming

	
	
	33
	LED3-W
	0-255
	LED3-white dimming

	
	31
	34
	LED4-R
	0-255
	LED4-Red dimming

	
	32
	35
	LED4-G
	0-255
	LED4-green dimming

	
	33
	36
	LED4-B
	0-255
	LED4-Blue dimming

	
	
	37
	LED4-W
	0-255
	LED4-white dimming

	
	34
	38
	LED5-R
	0-255
	LED5-Red dimming

	
	35
	39
	LED5-G
	0-255
	LED5-green dimming

	
	36
	40
	LED5-B
	0-255
	LED5-Blue dimming

	
	
	41
	LED5-W
	0-255
	LED5-white dimming

	
	37
	42
	LED6-R
	0-255
	LED6-Red dimming

	
	38
	43
	LED6-G
	0-255
	LED6-Green dimming

	
	39
	44
	LED6-B
	0-255
	LED6-Blue dimming

	
	
	45
	LED6-W
	0-255
	LED6-white dimming

	
	40
	46
	LED7-R
	0-255
	LED7-Red dimming

	
	41
	47
	LED7-G
	0-255
	LED7-green dimming

	
	42
	48
	LED7-B
	0-255
	LED7-Blue dimming

	
	
	49
	LED7-W
	0-255
	LED7-white dimming

	
	43
	50
	LED8-R
	0-255
	LED8-Red dimming

	
	44
	51
	LED8-G
	0-255
	LED8-green dimming

	
	45
	52
	LED8-B
	0-255
	LED8-Blue dimming

	
	
	53
	LED8-W
	0-255
	LED8-white dimming

	
	46
	54
	LED9-R
	0-255
	LED9-Red dimming

	
	47
	55
	LED9-G
	0-255
	LED9-green dimming

	
	48
	56
	LED9-B
	0-255
	LED9-Blue dimming

	
	
	57
	LED9-W
	0-255
	LED9-white dimming

	
	49
	58
	LED10-R
	0-255
	LED10-Red dimming

	
	50
	59
	LED10-G
	0-255
	LED10-Green dimming

	
	51
	60
	LED10-B
	0-255
	LED10-Blue dimming

	
	
	61
	LED10-W
	0-255
	LED10-white dimming

	
	52
	62
	LED11-R
	0-255
	LED11-Red dimming

	
	53
	63
	LED11-G
	0-255
	LED11-Green dimming

	
	54
	64
	LED11-B
	0-255
	LED11-Blue dimming

	
	
	65
	LED11-W
	0-255
	LED11-White dimming

	
	55
	66
	LED12-R
	0-255
	LED12-Red dimming

	
	56
	67
	LED12-G
	0-255
	LED12-Green dimming

	
	57
	68
	LED12-B
	0-255
	LED12-Blue dimming

	
	
	69
	LED12-W
	0-255
	LED12-white dimming

	
	58
	70
	LED13-R
	0-255
	LED13-Red dimming

	
	59
	71
	LED13-G
	0-255
	LED13-Green dimming

	
	60
	72
	LED13-B
	0-255
	LED13-Blue dimming

	
	
	73
	LED13-W
	0-255
	LED13-White dimming

	
	61
	74
	LED14-R
	0-255
	LED14-Red dimming

	
	62
	75
	LED14-G
	0-255
	LED14-Green dimming

	
	63
	76
	LED14-B
	0-255
	LED14-Blue dimming

	
	
	77
	LED14-W
	0-255
	LED14-white dimming

	
	64
	78
	LED15-R
	0-255
	LED15-Red dimming

	
	65
	79
	LED15-G
	0-255
	LED15-Green dimming

	
	66
	80
	LED15-B
	0-255
	LED15-Blue dimming

	
	
	81
	LED15-W
	0-255
	LED15-white dimming

	
	67
	82
	LED16-R
	0-255
	LED16-Red dimming

	
	68
	83
	LED16-G
	0-255
	LED16-Green dimming

	
	69
	84
	LED16-B
	0-255
	LED16-Blue dimming

	
	
	85
	LED16-W
	0-255
	LED16-white dimming

	
	70
	86
	LED17-R
	0-255
	LED17-Red dimming

	
	71
	87
	LED17-G
	0-255
	LED17-Green dimming

	
	72
	88
	LED17-B
	0-255
	LED17-Blue dimming

	
	
	89
	LED17-W
	0-255
	LED17-white dimming

	
	73
	90
	LED18-R
	0-255
	LED18-Red dimming

	
	74
	91
	LED18-G
	0-255
	LED18-Green dimming

	
	75
	92
	LED18-B
	0-255
	LED18-Blue dimming

	
	
	93
	LED18-W
	0-255
	LED18-white dimming

	
	76
	94
	LED19-R
	0-255
	LED19-Red dimming

	
	77
	95
	LED19-G
	0-255
	LED19-Green dimming

	
	78
	96
	LED19-B
	0-255
	LED19-Blue dimming

	
	
	97
	LED19-W
	0-255
	LED19-white dimming


	 channel 
	 function 
	DMX numeric value 
	 description 

	1
	1
	 red 
	0-255
	Linear dimming from dark to light

	2
	2
	Red tweaks
	0-255
	Red 16bit dimming

	3
	3
	 green 
	0-255
	Linear dimming from dark to light

	4
	4
	Green tweaks
	0-255
	Green 16bit dimming

	5
	5
	 blue 
	0-255
	Linear dimming from dark to light

	6
	6
	Blue fine-tuning
	0-255
	Blue 16bit dimming

	7
	7
	 white 
	0-255
	Linear dimming from dark to light

	8
	8
	White fine-tuning
	0-255
	White 16bit dimming

	9
	9
	Color temperature adjustment
	0-255
	8000K-2500K

	10
	10
	Color macro
	0-255
	10-120 valid 

	11
	11
	 stroboflash 
	0-255
	 stroboflash 

	12
	12
	General dimming
	0-255
	Linear dimming from dark to light

	13
	13
	General dimming fine-tuning
	0-255
	Total dimming 16bit

	14
	14
	X axle 
	0-255
	0-540 degrees

	15
	15
	X-axis fine-tuning
	0-255
	16-bit adjustable

	16
	16
	Y axle 
	0-255
	0-205 degrees

	17
	17
	Y-axis fine-tuning
	0-255
	16-bit adjustable

	18
	18
	 macro 
	0-255
	

	19
	19
	 reset 
	0-25
	Reset and clear 0

	
	
	
	26-76
	The effect motor resets

	
	
	
	77-127
	XY motor reset

	
	
	
	128-255
	All motors reset

	20
	20
	 amplify 
	0-255
	The Angle is adjusted linearly from small to large

	21
	21
	 revolve 
	0-127
	0-60 degrees

	
	
	
	128-188
	Counterclockwise from fast to slow

	
	
	
	189-193
	 cease 

	
	
	
	194-255
	Clockwise from slow to fast

	22
	22
	 effect 
	0-7
	Dimming mode

	
	
	
	August 14
	Static effects (one effect per number)

	
	
	
	15-70
	Dynamic effects (one effect per number)

	23
	23
	Effect speed
	0-63
	 cease 

	
	
	
	64-158
	The effect reverses from fast to slow

	
	
	
	159-160
	The effect is paused

	
	
	
	161-255
	The effect turns from slow to fast

	24
	24
	The effect fades
	0-255
	From fast to slow

	25
	25
	The effect is red
	0-255
	Red is linearly dimmed from dark to light

	26
	26
	The effect is green
	0-255
	The green is linearly dimmed from dark to bright

	27
	27
	The effect is blue
	0-255
	The blue is linearly dimmed from dark to light

	28
	28
	The effect is white
	0-255
	The white is linearly dimmed from dark to light

	29
	29
	Adjust the light
	0-255
	Effect foreground color dimming

	30
	30
	Background dimming
	0-255
	Adjust the background color of the effect

	31
	31
	The effect transitions
	0-255
	

	32
	32
	Effect enhancements
	0-255
	

	33
	33
	The prospects are flashing
	0-255
	The effect is frequent flashing

	34
	34
	Background strobe
	0-255
	The effect is to flash the scene

	35
	35
	 background selection 
	0-255
	

	
	36
	LED1-R
	0-255
	LED1-Red dimming

	
	37
	LED1-G
	0-255
	LED1-Green dimming

	
	38
	LED1-B
	0-255
	LED1-Blue dimming

	
	39
	LED2-R
	0-255
	LED2-Red dimming

	
	40
	LED2-G
	0-255
	LED2-Green dimming

	
	41
	LED2-B
	0-255
	LED2-Blue dimming

	
	42
	LED3-R
	0-255
	LED3-Red dimming

	
	43
	LED3-G
	0-255
	LED3-green dimming

	
	44
	LED3-B
	0-255
	LED3-Blue dimming

	
	45
	LED4-R
	0-255
	LED4-Red dimming

	
	46
	LED4-G
	0-255
	LED4-green dimming

	
	47
	LED4-B
	0-255
	LED4-Blue dimming

	
	48
	LED5-R
	0-255
	LED5-Red dimming

	
	49
	LED5-G
	0-255
	LED5-green dimming

	
	50
	LED5-B
	0-255
	LED5-Blue dimming

	
	51
	LED6-R
	0-255
	LED6-Red dimming

	
	52
	LED6-G
	0-255
	LED6-Green dimming

	
	53
	LED6-B
	0-255
	LED6-Blue color dimming

	
	54
	LED7-R
	0-255
	LED7-Red dimming

	
	55
	LED7-G
	0-255
	LED7-green dimming

	
	56
	LED7-B
	0-255
	LED7-Blue dimming

	
	57
	LED8-R
	0-255
	LED8-Red dimming

	
	58
	LED8-G
	0-255
	LED8-green dimming

	
	59
	LED8-B
	0-255
	LED8-Blue dimming

	
	60
	LED9-R
	0-255
	LED9-Red dimming

	
	61
	LED9-G
	0-255
	LED9-green dimming

	
	62
	LED9-B
	0-255
	LED9-Blue dimming

	
	63
	LED10-R
	0-255
	LED10-Red dimming

	
	64
	LED10-G
	0-255
	LED10-Green dimming

	
	65
	LED10-B
	0-255
	LED10-Blue dimming

	
	66
	LED11-R
	0-255
	LED11-Red dimming

	
	67
	LED11-G
	0-255
	LED11-Green dimming

	
	68
	LED11-B
	0-255
	LED11-Blue dimming

	
	69
	LED12-R
	0-255
	LED12-Red dimming

	
	70
	LED12-G
	0-255
	LED12-Green dimming

	
	71
	LED12-B
	0-255
	LED12-Blue dimming

	
	72
	LED13-R
	0-255
	LED13-Red dimming

	
	73
	LED13-G
	0-255
	LED13-Green dimming

	
	74
	LED13-B
	0-255
	LED13-Blue dimming

	
	75
	LED14-R
	0-255
	LED14-Red dimming

	
	76
	LED14-G
	0-255
	LED14-Green dimming

	
	77
	LED14-B
	0-255
	LED14-Blue dimming

	
	78
	LED15-R
	0-255
	LED15-Red dimming

	
	79
	LED15-G
	0-255
	LED15-Green dimming

	
	80
	LED15-B
	0-255
	LED15-Blue dimming

	
	81
	LED16-R
	0-255
	LED16-Red dimming

	
	82
	LED16-G
	0-255
	LED16-Green dimming

	
	83
	LED16-B
	0-255
	LED16-Blue dimming

	
	84
	LED17-R
	0-255
	LED17-Red dimming

	
	85
	LED17-G
	0-255
	LED17-Green dimming

	
	86
	LED17-B
	0-255
	LED17-Blue dimming

	
	87
	LED18-R
	0-255
	LED18-Red dimming

	
	88
	LED18-G
	0-255
	LED18-Green dimming

	
	89
	LED18-B
	0-255
	LED18-Blue dimming

	
	90
	LED19-R
	0-255
	LED19-Red dimming

	
	91
	LED19-G
	0-255
	LED19-Green dimming

	
	92
	LED19-B
	0-255
	LED19-Blue dimming




	CH23
	CH99
	 function 
	DMX numeric value 
	 description 

	1
	1
	X axle 
	0-255
	 horizontal control 

	2
	2
	X-axis fine-tuning
	0-255
	Level fine-tuning control

	3
	3
	Y axle 
	0-255
	 vertical control 

	4
	4
	Y-axis fine-tuning
	0-255
	Vertical fine-tuning control

	5
	5
	XY velocity 
	0-255
	The horizontal/vertical speed is from fast to slow

	6
	6
	 focus 
	0-255
	 focus 

	7
	7
	 tilting mirror 
	0-127
	0 to 60 degrees

	
	
	
	128-188
	Counterclockwise from fast to slow infinity

	
	
	
	189-193
	 cease 

	
	
	
	194-255
	Turn clockwise from slow to fast infinitely

	8
	8
	 aiming 
	0-255
	Linear dimming from dark to light

	9
	9
	 stroboflash 
	0-3
	 light up 

	
	
	
	4-200
	The synchronous flicker speed is from slow to fast (1HZ-25HZ)

	
	
	
	201-215
	Low speed random flash

	
	
	
	216-234
	Medium speed random flashing

	
	
	
	235-255
	High speed random flash

	10
	10
	 red 
	0-255
	Red is linearly dimmed from dark to light

	11
	11
	 green 
	0-255
	The green is linearly dimmed from dark to bright

	12
	12
	 blue 
	0-255
	The blue is linearly dimmed from dark to light

	13
	13
	 white 
	0-255
	The white is linearly dimmed from dark to light

	14
	14
	Color temperature adjustment
	0-255
	Linear color temperature adjustment

	15
	15
	Color macro
	0-255
	Built-in color gradient

	16
	16
	Static effects
	0-9
	 not have 

	
	
	
	10-14
	Static effect 1

	
	
	
	15-19
	Static effect 2

	
	
	
	20-24
	Static effect 3

	
	
	
	...

	
	
	
	Five numbers make one effect

	
	
	
	...

	
	
	
	175-179
	Static effect 34

	
	
	
	180-184
	Static effect 35

	
	
	
	185-255
	Static effect 36

	17
	17
	Dynamic effects
	0-9
	 not have 

	
	
	
	10-14
	Effect 1

	
	
	
	15-19
	Effect 2

	
	
	
	20-24
	Effect 3

	
	
	
	...
	...

	
	
	
	Five numbers make one effect

	
	
	
	220-224
	Effect 43

	
	
	
	225-229
	Effect 44

	
	
	
	230-255
	Effect 45

	18
	18
	Dynamic effect speed
	0-126
	The positive direction is from fast to slow

	
	
	
	127-128
	 static 

	
	
	
	129-255
	The reverse goes from slow to fast

	19
	19
	Background red
	0-255
	The background effect red is linearly dimmed from dark to bright

	20
	20
	Background green
	0-255
	The background effect is a linear dimming of the green color from dark to light

	21
	21
	Background is blue
	0-255
	The background effect is linearly dimmed from dark to light blue

	22
	22
	Background white
	0-255
	The background effect is linearly dimmed from dark to light

	23
	23
	 reset 
	0-26
	 not have 

	
	
	
	27-76
	The lamp head is reset for 5 seconds

	
	
	
	77-127
	XY reset is effective for 5s

	
	
	
	128-255
	Full reset is valid for 5 seconds

	/
	24
	R1 LED dimming
	0-255
	R1 LED dimming

	
	25
	G1 LED dimming
	0-255
	G1 LED dimming

	
	26
	B1 LED dimming
	0-255
	B1 LED dimming

	
	27
	W1 LED dimming
	0-255
	W1 LED dimming

	
	…
	…
	……
	……

	
	…
	…
	……
	……

	
	96
	R19 LED dimming
	0-255
	R19 LED dimming

	
	97
	G19 LED dimming
	0-255
	G19 LED dimming

	
	98
	B19 LED dimming
	0-255
	B19 LED dimming

	
	99
	W19 LED dimming
	0-255
	W19 LED dimming




9. Product maintenance and cleaning
Please pay attention to the following points when testing this product:
1. All screws and parts of the installed products must be tightly connected and not rust.
2. The shell, lens, fasteners and installation locations (e.g. ceiling, bracket, truss, etc.) shall not deform.
3. The mechanical moving parts should not be worn and should not rotate unbalanceably.
4. The power cord should not be damaged in any way, such as material damage or scratches.
[image: 222]The installation and use of the products must be carried out by trained professional technicians to ensure that safety risks are eliminated.



In order to maintain the good condition of the product and extend its service life, we recommend regular cleaning of the product.
1. Clean the external lens and internal lens of the product every week to prevent the light output of the product from being weakened due to dust accumulation on the lens.
2. Clean the fan every week.
3. Professional electrical engineers shall conduct detailed circuit inspection on the products every three months to ensure good circuit joints and prevent aging of circuit joints due to overheating.
We recommend that the product should be cleaned regularly. Please note that do not use wet or linen cloth, and do not use alcohol or solvent for cleaning.
This product does not come with replacement parts. Please refer to the "Installation Instructions" section.
If you need any spare parts, please purchase them from your local dealer.
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