Three eye color light instruction manual
As the product is constantly updated, the content of this manual may be slightly different from the actual product, please forgive!
 product summary 
Display the button function of the panel
Menu functions
Channel description
Common function usage
Master/slave function
Vi. Technical parameters:
1. Display panel operation instructions
After starting up, press the MENU key to switch the menu, press the UP key (UP) or the DOWN key (DOWN) to select the setting value. After setting, press the ENTER key to confirm and save, and the display will flash once to indicate that the data is saved.
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Menu Up Down OK
Key function:
Menu key (MENU): Select the functions
Up (UP): Function parameter increment selection
Down (DOWN): Decreasing selection of function parameters
Confirm (ENTER): Confirm the current menu
Second, menu function
After powering on and turning the device on, press the MENU key to select the following functions. If you need a specific function, press the confirm button to confirm it. (This sequence applies to new machines. If the lamp was previously used in another mode and this mode was saved before shutdown, it will revert to the last saved mode upon reboot.) After setting other functions, press the confirm button to save your changes; otherwise, the settings from the last shutdown will not be retained when you restart the device
	A001
	 SHAPE  \* MERGEFORMAT 



	A512
	 SHAPE  \* MERGEFORMAT 



	In 10-channel mode, press the up or down key to select the address code (A001~A512), and press the confirm key to save the address code

	d001
	 SHAPE  \* MERGEFORMAT 



	F512
	 SHAPE  \* MERGEFORMAT 



	In mode 6, press the up or down key to select the address code (d001~d512), and press the confirm key to save the address code

	FF00
	 SHAPE  \* MERGEFORMAT 



	FF99
	 SHAPE  \* MERGEFORMAT 



	In the gradient mode, select the running speed (FF00-FF99) by pressing the up or down key, and save the current running speed by pressing the confirm key.

	EE00
	 SHAPE  \* MERGEFORMAT 



	EE99
	 SHAPE  \* MERGEFORMAT 



	In pulse mode, press the up or down key to select the running speed (EE00-EE99), and press the confirm key to save the current running speed.

	CC00
	 SHAPE  \* MERGEFORMAT 
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	 SHAPE  \* MERGEFORMAT 



	In the jump mode, press the up or down key to select the running speed (CC00-CC99), and press the confirm key to save the current running speed.
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	Voice-activated mode

	R255
	 SHAPE  \* MERGEFORMAT 
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	 SHAPE  \* MERGEFORMAT 



	For manual W1 adjustment, press the up or down key between R000 and R255 to adjust the brightness without a console, and press the confirm key to save.

	G255
	 SHAPE  \* MERGEFORMAT 



	G001
	 SHAPE  \* MERGEFORMAT 



	Manual Y1 adjustment: when there is no console, press the up or down key to adjust the brightness between G000 and G255, and press the confirm key to save.

	B255
	 SHAPE  \* MERGEFORMAT 
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	 SHAPE  \* MERGEFORMAT 



	Manual W2 adjustment: when there is no console, press the up or down key to adjust the brightness between B000 and B255, and press the confirm key to save.

	W255
	 SHAPE  \* MERGEFORMAT 



	W001
	 SHAPE  \* MERGEFORMAT 



	For manual Y2 adjustment, press the up or down key between W000 and W255 to adjust the brightness without a console, and press the confirm key to save.

	Y255
	 SHAPE  \* MERGEFORMAT 



	Y001
	 SHAPE  \* MERGEFORMAT 



	For manual W3 adjustment, press the up or down key to adjust the brightness between Y000 and Y255 when there is no console, and press the confirm key to save

	P255
	 SHAPE  \* MERGEFORMAT 



	I001
	 SHAPE  \* MERGEFORMAT 



	Manual Y3 adjustment: when there is no console, press up or down key to adjust the brightness between I000 and I255, and press the confirm key to save

	F000
	
	F105
	
	Temperature display


Channel description (A001 and d001 channel value description)
Channel A001 description
	10 channel 
	
	Channel values
	 function 

	1
	General dimming
	000-255
	From dark to light

	2
	 stroboflash 
	000-255
	0-9 Invalid
10-255 from slow to fast

	3
	Built-in mode
	0-99
	Dimming mode

	
	
	100-149
	Gradient mode

	
	
	150-199
	Pulse variation mode

	
	
	200-229
	Jump mode

	
	
	230-255
	Voice control: The pace of light changes depends on the MIC of each lamp (i.e. cannot be guaranteed to synchronize)

	4
	Built-in mode speed
	000-255
	From slow to fast

	5
	W1
	000-255
	The brightness is adjusted from dark to bright

	6
	Y1
	000-255
	The brightness is adjusted from dark to bright

	7
	W2
	000-255
	The brightness is adjusted from dark to bright

	8
	Y2
	000-255
	The brightness is adjusted from dark to bright

	9
	W3
	000-255
	The brightness is adjusted from dark to bright

	10
	Y3
	000-255
	The brightness is adjusted from dark to bright


D001 Channel value description
	6 channel 
	
	Channel values
	 function 

	1
	W1
	000-255
	The brightness is adjusted from dark to bright

	2
	Y1
	000-255
	The brightness is adjusted from dark to bright

	3
	W2
	000-255
	The brightness is adjusted from dark to bright

	4
	Y2
	000-255
	The brightness is adjusted from dark to bright

	5
	W3
	000-255
	The brightness is adjusted from dark to bright

	6
	Y3
	000-255
	The brightness is adjusted from dark to bright


Fourth, use of common functions
1. DMX512 control
After powering on, set the digital display panel to A001 or d001, then connect the control panel to the PA light using a signal line. Once connected, the PA light digital display panel will not flicker if it receives the 512 signal. If the digital display panel continues to flicker, it indicates that the LED PA light has not received the 512 signal. Check the lighting fixtures, signal lines, and control panel for any issues. As long as the address code is correctly set, the LED PA light can be controlled using the 512 control panel.
2, FF00 (gradient mode), EE00 (pulse mode), CC00 (jump mode), Soud (voice control mode), as long as the menu is called out, press the confirm key to use the relevant function pull.
Five, master and slave machine setting
Two or more identical lamps are connected with a 3-core signal line. Set any host to sound control or gradient, pulse change, jump change, and other lamps in A001 or d001 mode, then enter the master-slave mode and the slave display screen does not flash (flashing indicates that the machine does not receive the signal, and the connection line must be checked)
Special note: Only one host can be set in a group of lamps. If there are multiple hosts, all lamps will flash randomly and step synchronously.
Vi. Technical parameters:
Voltage: AC100~240V 50/60HZ
Power: 150W
Lighting beads: 3 *50W2 one white and warm white light beads,
Control mode: DMX512, self-walking, master and slave.
 channel ：10CH、06CH、
Dimming: 32bit linear dimming from 0 to 100%
Features: front light + flash + point control
Working temperature: -30 ~80 degrees
Flicker frequency: 1~30HZ
Appearance: metal, black
Connection mode: DMX512 input/output / power input/output.
IP class: IP20
Size: Weight:                                Size: Weight:
