Specification of projection lamp
First of all, thank you for using our products. It uses the most advanced light source in the world - cold LED as the light source, which overcomes the shortcomings of traditional light sources, such as high power consumption, short service life and high temperature. It has the characteristics of low power consumption, long service life (generally up to about 60000 hours), high brightness and bright colors.It is an ideal product for stage lighting and various effect decoration.
 
 
1、 Operation instructions of display board
After starting up, press the menu key (menu key) to switch the menu, press the up key or down key to select the set value. After setting, press the Enter key to save and the display will flash to indicate that the data is saved.
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 Menu up and down confirmation
Basic usage:
Menu key: select various functions
Up: function parameters are selected step by step
Down: function parameter decreasing selection
Confirm (): confirm the current menuENTER
 
2、 Menu function
After power on, press the menu key (menu key) to successively display the following functions, and then press the OK key to confirm.(this sequence is the sequence of the new machine. If the lamp has used other modes and saved this mode before shutdown, the mode before the last shutdown will be displayed after starting up again). After setting other functions, you also need to press the save key to save, otherwise the effect of setting before shutdown will not appear after starting up next time
	A001
	8In channel mode, press up / down to select the address code (A001 ~ A512), and press enter to save the address code

	L001
	4In channel mode, press up / down to select the address code (D001 ~ D512), and press enter to save the address code

	d001
	2In channel mode, press up / down to select the address code (D001 ~ D512), and press enter to save the address code

	M000
	M000
	Dimming

	
	M001
	Not bright

	
	M002
	Light bead R is on

	
	M003
	Light bead G is on

	
	M004
	Light bead, G, R

	
	M005
	Light bead B is on

	
	M006
	Light beads R and B are on

	
	M007
	Light beads g and B are on

	
	M008
	Light beads R, G, B, on

	
	M009
	Light bead w on

	
	M010
	Light beads R and W are on

	
	M011
	Light beads g and W are on

	
	M012
	Light beads R, G and W are on

	
	M013
	Light beads B and W are on

	
	M014
	Light beads R, B and W are on

	
	M015
	Light beads g, B and W are on

	
	M016
	Light beads R, G, B and W are on

	
	M017
	Gradual change

	
	M018
	Pulse change

	
	M019
	Lamp bead R → g → B → w circulating light

	
	M020
	Lamp bead w → B → G-R cycle lamp

	
	M021
	Lamp beads R, G, and B, w cycle light

	
	M022
	Lamp beads R, W and G, B cycle running lamp

	
	M023
	Lamp beads R, B, and G, W, cycle lamp

	
	M024
	Lamp beads R, G to g, B to B, w to W, R cycle light

	
	M025
	Lamp beads R, G, B to g, B, w to B, W, R, cycle light

	
	M026
	Lamp bead r-g-b-w circulation

	
	M027
	Voice control

	S000
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	S255
	For stroboscopic speed adjustment, press up / down to adjust between s000-s255Press enter to save the speed.

	P000
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	P255
	Function mode self walking speed (M000 mode), press the up key / down key to adjust between r000-r255.Press enter to save the speed.

	R001
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	R255
	Manually r brightness, when there is no console, press the up / down key to adjust the brightness between r000-r255, and press the Enter key to save the brightness.

	G001
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	G255
	Manually g brightness, when there is no console, press the up / down key to adjust the brightness between g000-g255, and press the Enter key to save the brightness.

	B001
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	B255
	Manually B brightness, when there is no console, press the up / down key to adjust the brightness between b000-b255, and press the Enter key to save the brightness.

	W001
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	W255
	Manually adjust the brightness. When there is no console, press the up / down key to adjust the brightness between w000-w255, and press the Enter key to save the brightness.


  
3、 A001 and L001 D001 channel value description
A001 eight channel description
	passageway
	Channel value
	function

	1
	000-255
	Total dimming, linear dimming, from dark to bright

	2
	000-255
	Total stroboscopic, from slow to fast

	3
	0-29
	Dimming

	
	30-34
	Not bright

	
	35-39
	Light bead R is on

	
	40-44
	Light bead G is on

	
	45-49
	Light beads R and G are on

	
	50-54
	Light bead B is on

	
	55-59
	Light beads R and B are on

	
	60-64
	Light beads g and B are on

	
	65-69
	Light beads R, G, B, on

	
	70-74
	Light bead w on

	
	76-79
	Light beads R and W are on

	
	80-84
	Light beads g and W are on

	
	85-89
	Light beads R, G and W are on

	
	90-94
	Light beads B and W are on

	
	95-99
	Light beads R, B and W are on

	
	100-104
	Light beads g, B and W are on

	
	115-109
	Light beads R, G, B and W are on

	
	110-139
	Gradual change

	
	140-169
	Pulse change

	
	170-179
	Lamp bead R → g → B → w circulating light

	
	180-189
	Lamp bead w → B → G-R cycle lamp

	
	190-199
	Lamp beads R, G, and B, w cycle light

	
	200-209
	Lamp beads R, W and G, B cycle running lamp

	 
	210-219
	Lamp beads R, B, and G, W, cycle lamp

	
	220-229
	Lamp beads R, G to g, B to B, w to W, R cycle light

	
	230-239
	Lamp beads R, G, B to g, B, w to B, W, R, cycle light

	
	240-249
	Lamp bead r-g-b-w circulation

	
	250-255
	Voice control

	4
	000-255
	Channel 3 function speed, from slow to fast

	5
	000-255
	R linear dimming, adjusting from dark to light.

	6
	000-255
	G linear dimming, adjusting from dark to light.

	7
	000-255
	B linear dimming, adjusting from dark to light.

	8
	000-255
	W linear dimming, adjustable from dark to light.


 L001 four channel value description
	passageway
	Channel value
	function

	1
	000-255
	Total dimming, linear dimming, from dark to bright

	2
	000-255
	RB linear dimming, adjusting from dark to light.

	3
	000-255
	GW linear dimming, adjusting from dark to light.

	4
	000-255
	Total stroboscopic, from slow to fast


 
D001 two channel value description
	passageway
	Channel value
	function

	1
	000-255
	Total dimming, linear dimming, from dark to bright

	2
	000-255
	Total stroboscopic, from slow to fast


 
 
4、 Master slave setting
2Two or more identical lamps are connected by 3-core signal wires. If any host is set as voice control or gradual change, pulse change and jump change, and other lamps are in A001 mode, it will enter the master-slave mode and the slave display screen will not flash (flashing indicates that the machine has not received a signal, and the connecting wire must be checked)
Special attention: only one host can be set in a group of lamps. If there are multiple hosts, all lamps will flash randomly and step synchronously.
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