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MANUAL DEL USUARIO

   Por  seguridad  y  una  mejor operación, por favor lea este manual cuidadosamente antes de usar y operar este equipo, para que no ocurra ninguna lesión personal ni daño a laluminaria.


Specifications  

. Input Voltage: 110-240V AC, 50-60 Hertz
. Max Power Consumption: 360W 
Light Source
. 24 x 15W LEDs(R,G,B,W)
Optical
. Lens Angle: 25° / 40°
Control Singal
. Protocol USITT DMX-512
. DMX Channels: 5/9
Cooling Method: Aluminum radiator
IP rate: IP20
Net Weight：4kgs
Dimension: 530×530×400mm / 4 pcs
Aviation box packaging

Menu

	passageway
	Channel value
	function

	1
	000-255
	Total dimming, linear dimming, from dark to bright

	2
	000-255
	Total stroboscopic, from slow to fast

	3
	0-29
	Dimming

	
	30-34
	Not bright

	
	35-39
	Light bead R is on

	
	40-44
	Light bead G is on

	
	45-49
	Light beads R and G are on

	
	50-54
	Light bead B is on

	
	55-59
	Light beads R and B are on

	
	60-64
	Light beads g and B are on

	
	65-69
	Light beads R, G, B, on

	
	70-74
	Light bead w on

	
	[bookmark: _GoBack]75-79
	Light beads R and W are on

	
	80-84
	Light beads g and W are on

	
	85-89
	Light beads R, G and W are on

	
	90-94
	Light beads B and W are on

	
	95-99
	Light beads R, B and W are on

	
	100-104
	Light beads g, B and W are on

	
	115-109
	Light beads R, G, B and W are on

	
	110-139
	Gradual change

	
	140-169
	Pulse change

	
	170-179
	Lamp bead R → g → B → w circulating light

	
	180-189
	Lamp bead w → B → G-R cycle lamp

	
	190-199
	Lamp beads R, G, and B, w cycle light

	
	200-209
	Lamp beads R, W and G, B cycle running lamp

	 
	210-219
	Lamp beads R, B, and G, W, cycle lamp

	
	220-229
	Lamp beads R, G to g, B to B, w to W, R cycle light

	
	230-239
	Lamp beads R, G, B to g, B, w to B, W, R, cycle light

	
	240-249
	Lamp bead r-g-b-w circulation

	
	250-255
	Voice control

	4
	000-255
	Channel 3 function speed, from slow to fast

	5
	000-255
	R linear dimming, adjusting from dark to light.

	6
	000-255
	G linear dimming, adjusting from dark to light.

	7
	000-255
	B linear dimming, adjusting from dark to light.

	8
	000-255
	W linear dimming, adjustable from dark to light.
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