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Read the instructions carefully before use

 essential parameter ：
Rated power: 150W.
Voltage/frequency: AC110-240V/50-60HZ wide voltage switching power supply, can meet the requirements of different countries in the world for voltage and frequency. It adopts high-tech constant current power board, stable output voltage and current, long working life, strong anti-interference ability.
Channels: 8 and 4 control channel modes.
Control mode: divided into DMX mode, random mode, self-walking mode and voice control mode.
Light source: high quality, high brightness brand LED light source, 3W RGBW full color.
Beam Angle: Optical lens, standard 25 degrees (optional), full, uniform, bright, pure color.
Mixing effect: the uniform RGBW infinite mixing system, which can form a very rich color. Each color can be controlled by DMX512 signal alone, and the mixing between colors can produce a colorful effect.
Special functions: built-in a variety of lighting effect programs, sound control synchronous operation.
Frequency flash: high speed electronic frequency flash can be up to 1-25 times/second or random frequency flash.
Light dimming: the total light dimming channel can control the brightness change and light closure of 5 main colors at the same time, and there is no flicker or jitter phenomenon.
Heat dissipation protection: high heat dissipation performance aluminum special self-cooling radiator without fan, high quality full pressure stretching aluminum shell, so that the heat of the lamp body is discharged in time, always kept in the predetermined temperature range, with temperature control protection function, silent and dust-free can extend the service life.
Design: beautiful and robust, with design patent, imitation must be investigated.
IP protection level: IP20;
Product size: 310*310*270 mm              Product size: 310*310*270 mm
Net weight: 5 Kg


1. Display menu and instructions


2.DMX channel table
(1) A001: Extended mode channel table
	 channel 
	Channel name
	 numeric value 
	 explain 

	1
	 aiming 
	0~255
	General dimming

	2
	 stroboflash 
	0~255
	From slow to fast flicker

	3
	Effect / mode
	0~5
	Manual color adjustment (red, green, blue......)

	
	
	6~50
	Gradual color change

	
	
	51~100
	Gradual color change

	
	
	101~150
	Twitch to change color

	
	
	151~200
	Automatic mode (ignoring data from other channels except this channel and speed channel)

	
	
	201~255
	Voice-activated mode (ignoring data from other channels except this channel and speed channel)

	4
	 velocity 
	0~255
	When [Effect/Mode] is enabled, adjust the speed of color change or self-walking

	5
	 red 
	0~255
	Linear dimming

	6
	 green 
	0~255
	Linear dimming

	7
	 blue 
	0~255
	Linear dimming

	8
	 white 
	0~255
	Linear dimming



(2) D001: Simple mode channel table
	 channel 
	Channel name
	 numeric value 
	 explain 

	1
	 red 
	0~255
	Linear dimming

	2
	 green 
	0~255
	Linear dimming

	3
	 blue 
	0~255
	Linear dimming

	4
	 white 
	0~255
	Linear dimming
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1. A001

2. d001

3. CC00

4. EE00

5. FF00

6. Ato0

7. Sou0

8. Col0

10. r000

11. G000

12. b000

13. w000

DMX

地址

: 1~512(

扩展模式

:8

通道

)

颜色跳变

 (0~99)

颜色渐变

 (0~99)

颜色脉变

 (0~99)

自走模式

(0~9)

声控模式

 (0~9)

选色

 (0~9)

红色

 (0~255)

绿色

 (0~255)

蓝色

 (0~255)

白色

 (0~255)

快捷菜单说明

MODE UP DOWN ENTER

1

2

3

4

5

6. SB00

频闪

 (0~99)

9. CUS1

调配颜色

(1~5)

5.CFG

6.STA

5.1UO

5.3IR

U25.3

欠压保护使能

过温保护使能

红外遥控使能

5.2OT

Under voltage

Over temperate

IR remote

2.LED

3.DSP

4.BLK

1.Syn

T32.5

7.RST

NO YES

1. 4

位

8

段数码管显示屏

2. MODE:  (1)

选取快捷菜单

; (2)

从其他显示状态返回 快捷菜单 状态

3. DOWN:  (1)

选择菜单

; (2)

设置参数

.

4. UP: (1)

选择菜单

; (2)

设置参数

.

5. ENTER:

确认键

,

功能

: (1)

进入主菜单或子菜单

; (2)

保存设置

.

DMX

地址

: 1~512(

简单模式

:4

通道

)

主

/

从机设置

OFF: 

从机

ON: 

主机

省电模式

反转显示

系统参数

当前电源电压

版本号

当前温度

: 32.5

度

复位

黑场设置

OFF: LED

显示屏一直显示

ON: 10

秒无操作

,

关闭

LED

显示屏

OFF: 

正常显示

ON: 

显示反转

OFF: 

关闭黑场功能

ON: 

开启黑场功能

. 

当断

开控台时

,

灯光全灭

扩展功能

当次开机时间

( 

可升级

 )

( 

升级需加硬件

 )

( 

升级需加硬件

 )

(

按

MODE

键切换

)


image1.png




oleObject1.bin
1. A001


2. d001


3. CC00


4. EE00


5. FF00


6. Ato0


7. Sou0


8. Col0


10. r000


11. G000


12. b000


13. w000


主/从机设置


OFF: 从机


ON: 主机


省电模式


反转显示


系统参数


当前电源电压


版本号


当前温度: 32.5度


颜色渐变 (0~99)


DMX地址: 1~512(扩展模式:8通道)


DMX地址: 1~512(简单模式:4通道)


颜色跳变 (0~99)


颜色脉变 (0~99)


自走模式(0~9)


声控模式 (0~9)


选色 (0~9)


红色 (0~255)


绿色 (0~255)


蓝色 (0~255)


白色 (0~255)


快捷菜单说明


2.LED


ON: 10秒无操作,关闭LED显示屏


OFF: 正常显示


T32.5


ON: 显示反转


7.RST


NO


YES


1. 4位8段数码管显示屏 


2. MODE:  (1)选取快捷菜单; (2)从其他显示状态返回 快捷菜单 状态


3. DOWN:  (1)选择菜单; (2)设置参数.


4. UP:          (1)选择菜单; (2)设置参数.


5. ENTER: 确认键,功能: (1)进入主菜单或子菜单; (2)保存设置.


OFF: 关闭黑场功能


ON:�

扩展功能


当次开机时间


( 可升级 )


( 升级需加硬件 )


( 升级需加硬件 )


(按MODE键切换)


3.DSP


4.BLK


1.Syn


黑场设置


OFF: LED显示屏一直显示


5.CFG


6.STA


5.1UO


5.3IR


U25.3


欠压保护使能


过温保护使能


红外遥控使能


5.2OT


Under voltage


Over temperate


IR remote


MODE


UP


DOWN


ENTER


1


2


3


4


5


6. SB00


频闪 (0~99)


9. CUS1


调配颜色(1~5)


复位



