LED 12x40W Zoom Moving Head
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Please Read the Instructions Carefully Before Use.

1. Basic parameters:

Voltage: 100V-240V  50-60Hz

LEDs: 12x40W (RGBW) LEDs
Maximum power: 490W

Color temperature: 2800K-8500K

Spot angle: 4.5°-45°

Control mode: DMX512, master-slave operation,

Overall control channel: can be customized

Point control channel mode: 19CH / 67CH

Support RDM function, DMX software upgrade function

Focusing: high-quiet motor precision focusing spot without jitter

Display: color LCD display, Chinese and English display, reverse display

Strobe: 1-20Hz

Dimming: 0-100% (16bit)

Working environment temperature: 00C-450C

Product size: 396*291*410

Net weight: 14KG
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1. Product Size:

2. Display description：
	Menu
	DMX Address
	001-512

	
	System Setup
	Run  Mode
	DMX/Auto 1/Auto 2/Sound

	
	
	Channel  Mode
	19 CH / 67CH

	
	
	Invert Pan
	ON/OFF

	
	
	Invert Tilt
	ON/OFF

	
	
	Hall Crct
	ON/OFF

	
	
	Encoder Crct
	ON/OFF

	
	
	Signal Keep
	ON/OFF

	
	
	Screen Saver
	ON/OFF

	
	
	Invert Screen
	Auto/ON/OFF

	
	
	Update slave
	ON/OFF

	
	
	Language
	中文/EN

	
	
	Load Default
	OK/Cancel

	
	Manual Drive

	
	Calibration
	PAN
	001-255

	
	
	TILT
	001-255

	
	
	Focus
	001-255

	
	
	Balance-Red
	001-255

	
	
	        Balance-Green
	001-255

	
	
	  Balance-Blue
	001-255

	
	
	   Balance-White
	001-255

	
	
	Power
	001-255

	
	
	Balance1-Red
	001-255

	
	
	......
	......

	
	
	Balance12-White
	001-255

	
	
	MIC
	001-255

	
	
	Change password

	
	System Reset
	Reset  Effect

	
	
	Reset  Scan

	
	
	Reset  All

	
	System Info
	Reset Info

	
	
	DMX  Date

	
	
	Sensor Info
	Hardware

	
	
	
	Software


3. Channel List:
	19/67CH
	FUNCTION
	VALUE
	FUNCTION 

	1
	1
	Pan
	0-255
	Pan  0-540 degrees

	2
	2
	Pan fine adjust
	0-255
	Pan fine adjust

	3
	3
	Tilt
	0-255
	Tilt  0-540 degrees

	4
	4
	Tilt fine adjust
	0-255
	Tilt fine adjust

	5
	5
	Pan/Tilt speed
	0-255
	Pan / Tilt speed from slow to fast

	6
	6
	Focus
	0-255
	5-60 degrees of focus

	7
	7
	Total dimming
	0-255
	0-100% linear dimming

	8
	8
	Strobe
	0-84
	Flash from slow to fast

	
	
	
	85–170
	Random strobe from slow to fast

	
	
	
	171-225
	Flash strobe from slow to fast

	9
	9
	R
	0-255
	Red 0-100% linear dimming

	10
	10
	G
	0-255
	Green 0-100% linear dimming

	11
	11
	B
	0-255
	Blue 0-100% linear dimming

	12
	12
	W
	0-255
	White 0-100% linear dimming

	13
	13
	Color temperature
	0-255
	Color temperature regulation

	14
	14
	Color macro function

（static state）
	0-127
	Macro function color gradient effect

	
	
	
	128-255
	Macro function color jump change

	15
	15
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Macro function dynamic effect
	0-20
	No function

	
	
	
	21-27
	Effect 1

	
	
	
	28-227
	One effect per 8 DMX values (25 types)

	
	
	
	228-255
	Effect 27

	16
	16
	Macro function effect speed
	0-255
	Macro speed from slow to fast

	17
	17
	Background color dimming
	0-255
	Background color dimming

	18
	18
	Background color
	0-30
	Red background color

	
	
	
	31-60
	Green background color

	
	
	
	61-92
	Blue background color

	
	
	
	93-123
	White background color

	
	
	
	124-154
	Yellow background color

	
	
	
	155-185
	Purple background color

	
	
	
	186-216
	Light blue background color

	
	
	
	217-255
	Background color all ON

	19
	19
	Reset
	0-244
	No function

	
	
	
	245-255
	Reset

	/
	20
	R 1
	0-255
	1st  R dimming

	
	21
	G 1
	0-255
	1st  G dimming

	
	22
	B 1
	0-255
	1st  B dimming

	
	23
	W 1
	0-255
	1st  W dimming

	
	…..
	…..
	………….
	………...

	
	…..
	…..
	………….
	………….

	
	64
	R12
	0-255
	12th R dimming

	
	65
	G 12
	0-255
	12th G dimming

	
	66
	B 12
	0-255
	12th B dimming

	
	67
	W 12
	0-255
	12th W dimming


