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PLEASE READ THIS CAREFULLY BEFORE USE

Skill parameters
Light Sources: 7x60W RGBW Original LED
Power Voltage: AC 100-240V, 50/60Hz, 500w 
Single LED power: 60W
Color: RGBW automatic correction 16.7 million pixels
Electronic dimmer:0～100% linear
[bookmark: Control]Control
DMX Channel: 23/35/51 Channel
Control Modes: DMX512
Software Upgrade: Firmware update via DMX link
[bookmark: Pan/Tilt]Pan/Tilt
Pan/Tilt: 540°

Construction
Display: LCD Display
Data In/Out socket: 3-pin XLR sockets Power Socket: Powercon in/out
Protection Rating: IP20

[bookmark: Features]Features

Motorized liner zoom system, 
zoom range: 4.5°~45° Outstanding color macro effect,CTO,Kaleido effects,led single controlled
Dimmer: 0~100% smooth dimming Variable strobe effects
Fast, quiet operation and flicker free
/ 270° Pan/Tilt Resolution: 16bit



















































	23
	reset
	0-199
	invalid

	
	
	200-205
	Reset after 5 seconds

	
	
	206-255
	invalid

	35 CH
	Channel
	DMX  Value
	Function

	1
	red
	0-255
	Red dimmer

	2
	Red fine
	0-255
	Red dimmer fine

	3
	green
	0-255
	Green dimmer

	4
	Green fine
	0-255
	Green dimmer fine

	5
	blue
	0-255
	Blue dimmer

	6
	Blue fine
	0-255
	Blue dimmer fine

	7
	white
	0-255
	White dimmer

	8
	White fine
	0-255
	White dimmer fine

	9
	CT
	0-255
	Linear CT control

	10
	Color Macro
	0-255
	Color Macro function

	11
	strobe
	0-3
	off

	
	
	4-103
	Synchronous strobe slow-fast  （1HZ-25HZ）

	
	
	104-107
	on

	
	
	108-207
	Divide strobe from slow-fast   （1HZ-25HZ）

	
	
	208-212
	on

	
	
	213-225
	Random strobe in low speed

	
	
	226-238
	Random strobe in middle speed

	
	
	239-251
	Random strobe in high speed

	
	
	252-255
	on

	12
	dimmer
	0-255
	Linear dimmer from dark-bright

	13
	Dimmer fine
	0-255
	Dimmer fine

	14
	pan
	0-255
	pan

	15
	Pan fine
	0-255
	Pan fine

	16
	tilt
	0-255
	tilt

	17
	Tilt fine
	0-255
	Tilt fine

	18
	function
	0-255
	




	19
	reset
	0-199
	invalid

	
	
	200-205
	Reset after 5 seconds

	
	
	206-255
	invalid

	20
	zoom
	0-255
	zoom

	21
	Lens rotating
	0-127
	0~60 degree

	
	
	128-191
	Forward limitless rotate

	
	
	192-255
	Reverse limitless rotate

	22
	pattern
	0-255
	Pattern rotate

	23
	Pattern speed
	0-255
	Pattern speed

	24
	Pattern effect fade
	0-255
	

	25
	Pattern effect R
	0-255
	

	26
	Pattern effect G
	0-255
	

	27
	Pattern effect B
	0-255
	

	28
	Pattern effect W
	0-255
	

	29
	Pattern dimmer
	0-255
	Pattern 0-100% dimmer

	30
	Background dimmer
	0-255
	Background 0-100% dimmer

	31
	Pattern transition
	0-255
	

	32
	Pattern angle 
	0-255
	Pattern design

	33
	Prospect strobe
	0-255
	Prospect strobe（with 11 chs）

	34
	Background strobe
	0-255
	Background strobe（with 11 chs）

	35
	Background selection
	0-255
	

	51 CH
	Channel
	DMX  Value
	Function

	1
	X
	0-255
	0-540 degree 

	2
	X fine
	0-255
	16 bit

	3
	Y
	0-255
	0-205 degree

	4
	Y fine
	0-255
	16 bit

	5
	XY speed
	0-255
	Fast-slow

	6
	zoom
	0-255
	Small-big

	7
	rotating
	0-127
	0~60 degree

	
	
	128-191
	Forward fast-slow




	7
	rotating
	200-255
	Reverse slow-fast

	8
	dimmer
	0-255
	Dark-bright

	9
	strobe
	0-3
	on

	
	
	4-200
	Synchronous strobe slow-fast  

	
	
	201-215
	Random strobe in low speed

	
	
	216-234
	Random strobe in midlle speed

	
	
	235-255
	Random strobe in high speed

	10
	R dimmer
	0-255
	

	11
	G dimmer
	0-255
	

	12
	B dimmer
	0-255
	

	13
	W dimmer
	0-255
	

	14
	CT
	0-255
	Linear CT control

	15
	Wash
	0-255
	

	16
	Static effect
	0-255
	5 no. One effect

	17
	Dynamic effect
	0-255
	5 no. One effect

	18
	Dynamic effect speed
	0-127
	Forward fast-slow

	
	
	128-255
	Reverse slow-fast

	19
	Background R
	0-255
	Dark-bright

	20
	Background G
	0-255
	Dark-bright

	21
	Background B
	0-255
	Dark-bright

	22
	Background W
	0-255
	Dark-bright

	23
	reset
	0-199
	invalid

	
	
	200-205
	Reset after 5s

	
	
	206-255
	invalid

	24
	R1 LED dimmer
	0-255
	R1 LED dimmer

	25
	G1 LED dimmer
	0-255
	G1 LED dimmer

	26
	B1 LED dimmer
	0-255
	B1 LED dimmer

	27
	W1 LED dimmer
	0-255
	W1 LED dimmer

	…
	…
	……
	……

	48
	R7 LED dimmer
	0-255
	R7 LED dimmer

	49
	G7 LED dimmer
	0-255
	G7 LED dimmer

	50
	B7 LED dimmer
	0-255
	B7 LED dimmer

	51
	W7LED dimmer
	0-255
	W7 LED dimmer




Channels List

	23 CH
	Channel
	DMX  Value
	Function

	1
	X
	0-255
	0-540 degree

	2
	X fine
	0-255
	16 bit

	3
	Y
	0-255
	0-205 degree

	4
	Y fine
	0-255
	16 bit

	5
	XY speed
	0-255
	Fast-slow

	6
	zoom
	0-255
	Angle from small-big

	7
	rotating
	0-127
	0~60 degree

	
	
	128-191
	Antiwise fast-slow

	
	
	200-255
	Forward slow-fast

	8
	dimmer
	0-255
	From dark-bright

	9
	strobe
	0-3
	on

	
	
	4-200
	Synchronous strobe from slow-fast

	
	
	201-215
	Random strobe in low speed

	
	
	216-234
	Random strobe in middle speed

	
	
	235-255
	Random strobe in high speed

	10
	R dimmer
	0-255
	From dark-bright

	11
	G dimmer
	0-255
	From dark-bright

	12
	B dimmer
	0-255
	From dark-bright

	13
	W dimmer
	0-255
	From dark-bright

	14
	CT
	0-255
	Linear CT control

	15
	wash
	0-255
	Inner color gradual change

	16
	Static effect
	0-255
	5 no. One effect

	17
	Dynamic effect
	0-255
	5 no. One effect

	18
	Dynamic effect speed
	0-127
	Forward from fast-slow

	
	
	128-255
	Reverse from slow-fast

	19
	Background R
	0-255
	Dark-bright

	20
	Background G
	0-255
	Dark-bright

	21
	Background B
	0-255
	Dark-bright

	22
	Background W
	0-255
	Dark-bright
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