	
	 tornado 
	
	

	1, working voltage: AC220V/50Hz

	2. Product power: 400W

	3. Light bead parameters: 560W RGBW light sources and 620W white light sources

	4. Control mode: DMX512 is commonly used in the world

	h

	6. Light dimming mode: 0~100% ultra-smooth light dimming

	7. Strobe: 25 times per second

	
	
	
	

	28 channel 
	 function 
	DMX numeric value 
	 description 

	1
	Y1 axis
	0-255
	0~180 degrees

	2
	Y2 axis
	0-255
	0~180 degrees

	3
	Y3 axis
	0-255
	0~180 degrees

	4
	Y4 axis
	0-255
	0~180 degrees

	5
	Y5 axis
	0-255
	0~180 degrees

	6
	Y-axis velocity
	0-255
	0~180 degrees

	7
	General dimming
	0-255
	From dark to light

	8
	 stroboflash 
	0-10
	 NF 

	
	
	11-255
	The flicker speed is from slow to fast (1HZ~25HZ)

	9 (When running the built-in effect, this channel is used for running color selection)
	Y1 axis lamp (running color)
	0-23
	Blow out the lights

	
	
	24-47
	 red 

	
	
	48-71
	 green 

	
	
	72-95
	 blue 

	
	
	96-119
	 white 

	
	
	120-143
	Red + green

	
	
	144-167
	Red + blue

	
	
	168-191
	Green + blue

	
	
	192-215
	Red + green + blue

	
	
	216-255
	Red + green + blue + white

	10
	Y2 axis lamp
	0-23
	Blow out the lights

	
	
	24-47
	 red 

	
	
	48-71
	 green 

	
	
	72-95
	 blue 

	
	
	96-119
	 white 

	
	
	120-143
	Red + green

	
	
	144-167
	Red + blue

	
	
	168-191
	Green + blue

	
	
	192-215
	Red + green + blue

	
	
	216-255
	Red + green + blue + white

	11
	Y3 axis lamp
	0-23
	Blow out the lights

	
	
	24-47
	 red 

	
	
	48-71
	 green 

	
	
	72-95
	 blue 

	
	
	96-119
	 white 

	
	
	120-143
	Red + green

	
	
	144-167
	Red + blue

	
	
	168-191
	Green + blue

	
	
	192-215
	Red + green + blue

	12
	Y4 axis lamp
	0-23
	Blow out the lights

	
	
	24-47
	 red 

	
	
	48-71
	 green 

	
	
	72-95
	 blue 

	
	
	96-119
	 white 

	
	
	120-143
	Red + green

	
	
	144-167
	Red + blue

	
	
	168-191
	Green + blue

	
	
	192-215
	Red + green + blue

	13
	Y5 axis lamp
	0-23
	Blow out the lights

	
	
	24-47
	 red 

	
	
	48-71
	 green 

	
	
	72-95
	 blue 

	
	
	96-119
	 white 

	
	
	120-143
	Red + green

	
	
	144-167
	Red + blue

	
	
	168-191
	Green + blue

	
	
	192-215
	Red + green + blue

	14
	General dimming
	0-255
	From dark to light

	15
	 stroboflash 
	0
	 NF 

	
	
	1-255
	The flicker speed is from slow to fast (1HZ~25HZ)

	16
	Y1 white light
	0-255
	From dark to light

	17
	Y2 white light
	0-255
	From dark to light

	18
	Y3 white light
	0-255
	From dark to light

	19
	Y4 white light
	0-255
	From dark to light

	20
	Y5 white light
	0-255
	From dark to light

	21
	Y6 white light
	0-255
	From dark to light

	22
	Motor running method
	
	X/Y, axis running method

	
	
	0‐15
	 await the opportune moment 

	
	
	16‐35
	Run 1

	
	
	36‐55
	Run 2

	
	
	56‐75
	Run 3

	
	
	76‐95
	Run 4

	
	
	96‐115
	Run 5

	
	
	116‐135
	Run 6

	
	
	136‐155
	Run 7

	
	
	156‐175
	Run 8

	
	
	176‐195
	Run 9

	
	
	196-215 Run 10
	Run 10

	
	
	216-235 Run 11
	Run 11

	
	
	236-255 Run 12
	Run 12

	23
	5 RGBW light effects display
	0-5
	 all-or-none 

	
	
	6-20
	Built-in effect 1

	
	
	21-34
	Built-in effect 2

	
	
	35-48
	Built-in effect 3

	
	
	49-62
	Built-in effect 4

	
	
	63-76
	Built-in effect 5

	
	
	77-90
	Built-in effect 6

	
	
	91-104
	Built-in effect 7

	
	
	105-118
	Built-in effect 8

	
	
	119-132
	Built-in effect 9

	
	
	133-146
	Built-in effect 10

	
	
	147-160
	Built-in effect 11

	
	
	161-174
	Built-in effect 12

	
	
	175-188
	Built-in effect 13

	
	
	189-202
	Built-in effect 14

	
	
	203-216
	Built-in effect 15

	
	
	217-255
	Built-in effect 16

	24
	 impression 
	0-23
	Blow out the lights

	
	
	24-47
	 red 

	
	
	48-71
	 green 

	
	
	72-95
	 blue 

	
	
	96-119
	 white 

	
	
	120-143
	Red + green

	
	
	144-167
	Red + blue

	
	
	168-191
	Green + blue

	
	
	192-215
	Red + green + blue

	
	
	216-255
	Red + green + blue + white

	25
	5 RGBW light effect speed
	0-255
	From slow to fast

	26
	6 white light effects are displayed
	0-5
	 all-or-none 

	
	
	6-34
	Built-in effect 1

	
	
	35-63
	Built-in effect 2

	
	
	64-92
	Built-in effect 3

	
	
	93-121
	Built-in effect 4

	
	
	122-150
	Built-in effect 5

	
	
	151-179
	Built-in effect 6

	
	
	180-208
	Built-in effect 7

	
	
	209-237
	Built-in effect 8

	
	
	238-255
	Built-in effect 9

	27
	6 white light effects speed
	0-255
	From slow to fast

	28
	 macro 
	0-229
	Lighting effect display function priority dimming

	
	
	230-240
	Reset, reset within 3S.

	
	
	241-255
	 NF 

	
	
	
	

	17 channel 
	 function 
	DMX numeric value 
	 description 

	1
	Y1 axis
	0-255
	0 to 90 degrees

	2
	Y2 axis
	0-255
	0 to 90 degrees

	3
	Y3 axis
	0-255
	0 to 90 degrees

	4
	Y4 axis
	0-255
	0 to 90 degrees

	5
	Y5 axis
	0-255
	0 to 90 degrees

	6
	Y-axis velocity
	0-255
	From fast to slow

	7
	General dimming
	0-255
	From dark to light

	8
	 stroboflash 
	0
	 NF 

	
	
	1-255
	The flicker speed is from slow to fast (1HZ~25HZ)

	9 (This channel is running color when the built-in program is running)
	Y1-Y5 axis lamp beads (running color)
	0-23
	Blow out the lights

	
	
	24-47
	 red 

	
	
	48-71
	 green 

	
	
	72-95
	 blue 

	
	
	96-119
	 white 

	
	
	120-143
	Red + green

	
	
	144-167
	Red + blue

	
	
	168-191
	Green + blue

	
	
	192-215
	Red + green + blue

	
	
	216-255
	Red + green + blue + white

	10
	Y1-Y6 white light
	0-255
	From dark to light

	11
	Motor running
	
	X/Y, axis running method

	
	
	0‐15
	 await the opportune moment 

	
	
	16‐35
	Run 1

	
	
	36‐55
	Run 2

	
	
	56‐75
	Run 3

	
	
	76‐95
	Run 4

	
	
	96‐115
	Run 5

	
	
	116‐135
	Run 6

	
	
	136‐155
	Run 7

	
	
	156‐175
	Run 8

	
	
	176‐195
	Run 9

	
	
	196-215 Run 10
	Run 10

	
	
	216-235 Run 11
	Run 11

	
	
	236-255 Run 12
	Run 12

	12
	5 RGBW light effects display
	0-5
	 all-or-none 

	
	
	6-20
	Built-in effect 1

	
	
	21-34
	Built-in effect 2

	
	
	35-48
	Built-in effect 3

	
	
	49-62
	Built-in effect 4

	
	
	63-76
	Built-in effect 5

	
	
	77-90
	Built-in effect 6

	
	
	91-104
	Built-in effect 7

	
	
	105-118
	Built-in effect 8

	
	
	119-132
	Built-in effect 9

	
	
	133-146
	Built-in effect 10

	
	
	147-160
	Built-in effect 11

	
	
	161-174
	Built-in effect 12

	
	
	175-188
	Built-in effect 13

	
	
	189-202
	Built-in effect 14

	
	
	203-216
	Built-in effect 15

	
	
	217-255
	Built-in effect 16

	13
	 impression 
	0-23
	Blow out the lights

	
	
	24-47
	 red 

	
	
	48-71
	 green 

	
	
	72-95
	 blue 

	
	
	96-119
	 white 

	
	
	120-143
	Red + green

	
	
	144-167
	Red + blue

	
	
	168-191
	Green + blue

	
	
	192-215
	Red + green + blue

	
	
	216-255
	Red + green + blue + white

	14
	5 RGBW light effect speed
	0-255
	From slow to fast

	15
	6 white light effects are displayed
	0-5
	 all-or-none 

	
	
	6-34
	Built-in effect 1

	
	
	35-63
	Built-in effect 2

	
	
	64-92
	Built-in effect 3

	
	
	93-121
	Built-in effect 4

	
	
	122-150
	Built-in effect 5

	
	
	151-179
	Built-in effect 6

	
	
	180-208
	Built-in effect 7

	
	
	209-237
	Built-in effect 8

	
	
	238-255
	Built-in effect 9

	16
	4 white light effects speed
	0-255
	

	17
	 macro 
	0-229
	Lighting effect display function priority dimming

	
	
	230-240
	Reset, reset within 3S.

	
	
	241-255
	 NF 

	
	
	
	

	13 channel 
	 function 
	DMX numeric value 
	 description 

	1
	Y1-Y5 axis
	0-255
	0 to 90 degrees

	2
	Y-axis velocity
	0-255
	0 to 90 degrees

	3
	General dimming
	0-255
	From dark to light

	4
	 stroboflash 
	0
	 NF 

	
	
	1-255
	The flicker speed is from slow to fast (1HZ~25HZ)

	5 (The channel is running color when the built-in program is running)
	Y1-Y5 axis lamp beads
	0-23
	Blow out the lights

	
	
	24-47
	 red 

	
	
	48-71
	 green 

	
	
	72-95
	 blue 

	
	
	96-119
	 white 

	
	
	120-143
	Red + green

	
	
	144-167
	Red + blue

	
	
	168-191
	Green + blue

	
	
	192-215
	Red + green + blue

	
	
	216-255
	Red + green + blue + white

	6
	Y1-Y6 white light
	0-255
	From dark to light

	7
	Motor running
	
	X/Y, axis running method

	
	
	0‐15
	 await the opportune moment 

	
	
	16‐35
	Run 1

	
	
	36‐55
	Run 2

	
	
	56‐75
	Run 3

	
	
	76‐95
	Run 4

	
	
	96‐115
	Run 5

	
	
	116‐135
	Run 6

	
	
	136‐155
	Run 7

	
	
	156‐175
	Run 8

	
	
	176‐195
	Run 9

	
	
	196-215 Run 10
	Run 10

	
	
	216-235 Run 11
	Run 11

	
	
	236-255 Run 12
	Run 12

	8
	5 RGBW light effects display
	0-5
	 all-or-none 

	
	
	6-20
	Built-in effect 1

	
	
	21-34
	Built-in effect 2

	
	
	35-48
	Built-in effect 3

	
	
	49-62
	Built-in effect 4

	
	
	63-76
	Built-in effect 5

	
	
	77-90
	Built-in effect 6

	
	
	91-104
	Built-in effect 7

	
	
	105-118
	Built-in effect 8

	
	
	119-132
	Built-in effect 9

	
	
	133-146
	Built-in effect 10

	
	
	147-160
	Built-in effect 11

	
	
	161-174
	Built-in effect 12

	
	
	175-188
	Built-in effect 13

	
	
	189-202
	Built-in effect 14

	
	
	203-216
	Built-in effect 15

	
	
	217-255
	Built-in effect 16

	9
	 impression 
	0-23
	Blow out the light

	
	
	24-47
	 red 

	
	
	48-71
	 green 

	
	
	72-95
	 blue 

	
	
	96-119
	 white 

	
	
	120-143
	Red + green

	
	
	144-167
	Red + blue

	
	
	168-191
	Green + blue

	
	
	192-215
	Red + green + blue

	
	
	216-255
	Red + green + blue + white

	10
	5 RGBW light effect speed
	0-255
	From slow to fast

	11
	6 white light effects are displayed
	0-5
	 all-or-none 

	
	
	6-34
	Built-in effect 1

	
	
	35-63
	Built-in effect 2

	
	
	64-92
	Built-in effect 3

	
	
	93-121
	Built-in effect 4

	
	
	122-150
	Built-in effect 5

	
	
	151-179
	Built-in effect 6

	
	
	180-208
	Built-in effect 7

	
	
	209-237
	Built-in effect 8

	
	
	238-255
	Built-in effect 9

	12
	6 white light effects speed
	0-255
	From slow to fast

	13
	 macro 
	0-229
	Lighting effect display function priority dimming

	
	
	230-240
	Reset, reset within 3S.

	
	
	241-255
	 NF 


