810-A394-1260 watt Thousand-armed Guanyin manual

Define the display panel and buttons
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Menu key: Enter/return to the main menu
Up arrow: menu function up selection / parameter increment
Down arrow: Menu function down selection/parameter decrement
Confirmation key: Select the menu function, and confirm and save when modifying the parameters of the menu function.
Menu function
After powering on and resetting the entire unit, press the menu key to enter the main menu (if you do not operate for 30 seconds, the system will exit). Refer to the main menu function table (which includes 5 main menu options). Use the up or down keys to navigate through the main menu. Press the confirm key to modify the function parameters of each menu item. After making changes, press the confirm key to save the current function parameters (saving will retain the memory after power loss).
	 primary menu 
	 submenu 
	Menu function description

	1. System Settings
	1. DMX address
	Up or down modify the DMX address code (address code is optional range 001-512), confirm key save, default 001.

	
	2. Y reversal
	Up or down modify Y reverse on/off, confirm key save, default off.

	
	3. No signal
	 zero clearing 

	
	4. Advanced Settings
	

	2. Operation mode

	1. Operation mode
	Select the running mode DMX/voice control/automatic up or down, confirm the key to save, default DMX.

	
	2. Channel selection
	Select the channel up or down CH20.CH169A.CH169B.CH53.CH101.CH155.CH179 confirm key to save, default CH20.

	
	3、Y
	Up or down modify the operating parameter value of Y motor (adjustable range 000-255), confirm the key to save, default 128.

	
	4. Y speed
	Up or down modify the speed operation parameter value of Y motor (adjustable range 000-255), confirm the key to save, default 128.

	
	5、Y pattern 
	Up or down modify the value of Y mode parameter (adjustable range 000-255), confirm the key to save, default 128.

	
	6. Y model amplitude
	Up or down modify the Y mode amplitude parameter value (adjustable range 000-255), confirm the key to save, default 128.

	
	7. Focus
	Up or down modify the operating parameter value of the focusing motor (adjustable range 000-255), confirm the key to save, default 255.

	
	8. General dimming
	Up or down modify the dimming parameter value (adjustable range 000-255), confirm the key to save, default 255.

	
	9. Strobe
	Up or down modify the flicker parameter value (adjustable range 000-255), confirm the key to save, default 000.

	
	10. Red
	Up or down modify the brightness of the red LED (adjustable range 000-255), confirm the key to save, default 255.

	
	11. Green
	Up or down modify the brightness of the green LED (adjustable range 000-255), confirm the key to save, default 255.

	
	12. Blue
	Up or down modify the brightness of the blue LED (adjustable range 000-255), confirm the key to save, default 255.

	
	13. White
	Up or down modify the brightness of the white LED (adjustable range 000-255), confirm the key to save, default 255.

	
	14、 pattern 
	Up or down modify the mode parameter value (adjustable range 000-255), confirm the key to save, default 255.

	
	15. Speed
	Up or down modify the speed parameter value (adjustable range 000-255), confirm the key to save, default 255.

	
	16. Background color
	Up or down modify the background color parameter value (adjustable range 000-255), confirm the key to save, default 255.

	
	17. Background tone light
	Up or down modify the background tone light parameter value (adjustable range 000-255), confirm the key to save, default 255.

	
	18. Reset
	Yes/no

	4. Display Settings
	1. Language selection
	Select Chinese /EN (English) up or down, confirm the key to save, default Chinese.

	
	2. Inverted display Settings
	Select the on/off reverse display setting up or down, confirm the key to save, and the default is off.

	
	3. Screen protection
	Select on or off to turn the screen saver on or off. Confirm the key to save, and it is on by default.

	
	4. Software version
	04XZ

	5. Factory setup
	Display to enter the password! Up or down to 138, and then press the confirm key to enter the factory Settings.
	1. Y1 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	2. F1 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	3. Y2 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	4. F2 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	5. Y3 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	6. F3 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	7. Y4 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	8. F4 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 128.

	
	
	9. Y5 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 128.

	
	
	10. F5 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	11. Y6 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 128.

	
	
	12. F6 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 128.

	
	
	13. Y7 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	14. F7 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	15. Y8 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 128.

	
	
	16. F8 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	17. Y9 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	18. F9 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	19. Y10 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	20. F10 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	21. Y11 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	22. Calibration of F11 axis
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	23. Y12 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	24. F12 axis calibration
	Up or down modify the parameter (range 000-255), confirm the key is saved, default is 128.

	
	
	25, Y axis travel
	Modify the Y travel parameter (range 000-255) up or down, and confirm the key to save, default 128.

	
	
	26. Focus travel
	Up or down modify the focusing stroke parameter (range 000-255), confirm the key to save, default 128.

	
	
	27. Red
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	Green
	Up or down modify the parameter (range 000-255), confirm the key to save, default 255.

	
	
	29. Blue
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	30. White
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	31. Red
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	32. Green
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	33. Blue
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	34. White
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	35. Red
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	36. Green
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	37. Blue
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	38. White
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	39. Red
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	40. Green
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	41. Blue
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	42. White
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	43. Red
	Modify the parameter up or down (range 000-255), confirm the key is saved, default 255.

	
	
	44. Green
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	45. Blue
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	46. White
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	47. Red
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	48. Green
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	49. Blue
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	50. White
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	51. Red
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	52. Green
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	53. Blue
	Modify the parameter up or down (range 000-255), confirm the key is saved, default 255.

	
	
	54. White
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	55. Red
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	56. Green
	Modify the parameter up or down (range 000-255), confirm the key save, default 255.

	
	
	57. Blue
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	58. White
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	59. Red
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	Green
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	61. Blue
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	62. White
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	63. Red
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	64. Green
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	65. Blue
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	66. White
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	67. Red
	Up or down modify the parameter (range 000-255), confirm the key save, default 255.

	
	
	68. Green
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	69. Blue
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	70. White
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	71. Red
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	72. Green
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	73. Blue
	Modify the parameter up or down (range 000-255), confirm the key to save, default 255.

	
	
	74. White
	Up or down modify the parameter (range 000-255), confirm the key is saved, default 255.

	
	
	75. LED direction
	Up or down modify the LED direction parameter (range 000-255), confirm the key to save, default 000.

	
	
	76. Current
	Up or down modify the current parameter (range 000-255), confirm the key to save, default 230.

	
	
	77、LOGO
	LOGO changing-over 

	
	
	78、 temperature 
	Temperature modification. Default 45

	
	
	79. Temperature control-fan
	Open/close

	
	
	80、LED
	LED sequence switching

	
	
	81, YF direction
	Modify the YF direction parameter (range 000-255) up or down, and confirm that the key is saved. The default value is 000.


3. Master and slave machine control
Two or more identical lamps are connected using DMX three-core signal cables. All lamps are assigned any address code from 001 to 512, with one lamp set as the master and the others as slaves. The slave displays do not flicker. When the master adjusts the effects such as gradient, pulse, jump, sound control, and self-walking, all slaves will synchronize these effects.
Special attention: 1. Only one host can be set for a group of lamps. If there are multiple hosts, all lamps will flash randomly and out of sync.
           2. All lamps must be turned off when the DMX512 control console is closed for the master and slave machines to function.
4. DMX512 control
After setting the address code of all lamps, connect all lamps in parallel with DMX three-core signal lines to DMX512 control console. The address code stops flashing, indicating that the signal from DMX512 control console has been sent to the lamps. Control relevant functions according to channel instructions using DMX512 control console.
Note: Thousand-armed Guanyin V12 upgrade menu Y mode amplitude is 0 and the same as before. Use Y fine-tuning to control the Y mode amplitude
The amplitude of the Y mode is 1-255. The function channel 205-255 controls the amplitude of the Y mode. The function channel 0-204 uses the menu to set the amplitude of the Y mode and controls the amplitude of the Y mode
CH20 Channel Description:
	 channel 
	Channel values
	 basic function 

	1
	000-255
	Y coarse adjustment (Y mode direction)

	2
	000-255
	Y micro-adjustment body (Y mode amplitude)

	3
	000-255
	Y speed (Y mode speed)

	4
	000-255
	Y model (Y effect amplitude)

	5
	000-255
	CTC

	6
	000-255
	Color macro

	7
	000-255
	 pattern 

	8
	000-255
	Built-in LED effects

	9
	000-255
	LED built-in effect speed

	10
	000-255
	LED built-in effect tail time

	11
	000-255
	LED background colour 

	12
	000-255
	LED background tone light

	13
	000-255
	 aiming 

	14
	000-255
	 stroboflash 

	15
	000-255
	Zoom in overall

	16
	000-255
	 function 

	17
	000-255
	Red (effect color selection)

	18
	000-255
	Green (effect color selection)

	19
	000-255
	Blue (effect color selection)

	20
	000-255
	White (effect color selection)


Channel CH53 description:
	 channel 
	Channel values
	 basic function 

	1
	000-255
	Y1 coarse adjustment (Y mode direction)

	2
	000-255
	Y1 fine-tuning 

	3
	000-255
	Y2 coarse adjustment (Y mode amplitude)

	4
	000-255
	Y2 fine-tuning 

	5
	000-255
	Y3 coarse adjustment

	6
	000-255
	Y3 fine-tuning 

	7
	000-255
	Y4 fine-tuning

	8
	000-255
	Y4 fine-tuning 

	9
	000-255
	Y5 coarse adjustment

	10
	000-255
	Y5 fine-tuning 

	11
	000-255
	Y6 coarse adjustment

	12
	000-255
	Y6 fine-tuning 

	13
	000-255
	Y7 coarse adjustment

	14
	000-255
	Y7 fine-tuning 

	15
	000-255
	Y8 coarse adjustment

	16
	000-255
	Y8 fine-tuning 

	17
	000-255
	Y9 coarse adjustment

	18
	000-255
	Y9 fine-tuning 

	19
	000-255
	Y10 coarse adjustment

	20
	000-255
	Y10 fine-tuning 

	21
	000-255
	Y11 is fine-tuned

	22
	000-255
	Y11 fine-tuning 

	23
	000-255
	Y12 is fine-tuned

	24
	000-255
	Y12 fine-tuning 

	25
	000-255
	Y speed (Y mode speed)

	26
	000-255
	Y pattern 

	27
	000-255
	CTC

	28
	000-255
	Color macro

	29
	000-255
	 pattern 

	30
	000-255
	Built-in LED effects

	31
	000-255
	LED built-in effect speed

	32
	000-255
	LED built-in effect tail time

	33
	000-255
	LED background colour 

	34
	000-255
	Lightly adjust the LED background color tone

	35
	000-255
	 aiming 

	36
	000-255
	 stroboflash 

	37
	000-255
	Zoom in 1

	38
	000-255
	Zoom in 2

	39
	000-255
	Zoom in 3

	40
	000-255
	Zoom in 4

	41
	000-255
	Zoom in 5

	42
	000-255
	Zoom in 6

	43
	000-255
	Zoom in 7

	44
	000-255
	Zoom in 8

	45
	000-255
	Zoom in 9

	46
	000-255
	Zoom in 10

	47
	000-255
	Zoom in 11

	48
	000-255
	Zoom in 12

	49
	000-255
	 function 

	50
	000-255
	 red 

	51
	000-255
	 green 

	52
	000-255
	 blue 

	53
	000-255
	 white 


Channel CH169A description:
	 channel 
	Channel values
	 basic function 

	1
	000-255
	 function 

	2
	000-255
	Y speed (Y mode speed)

	3
	000-255
	Y pattern 

	4
	000-255
	CTC

	5
	000-255
	Color macro

	6
	000-255
	 pattern 

	7
	000-255
	Built-in LED effects

	8
	000-255
	LED built-in effect speed

	9
	000-255
	LED built-in effect tail time

	10
	000-255
	LED background colour 

	11
	000-255
	Lightly adjust the LED background color tone

	12
	000-255
	LED background tone light fine tuning

	13
	000-255
	 stroboflash 

	14
	000-255
	Y1 coarse adjustment (Y mode direction)

	15
	000-255
	Y1 fine-tuning 

	16
	000-255
	Zoom in 1

	17
	000-255
	Dimming 1 coarse adjustment

	18
	000-255
	Dimming 1 fine adjustment

	19
	000-255
	Red 1 is a coarse adjustment

	20
	000-255
	Red 1 fine-tuning

	21
	000-255
	Green 1 is a coarse adjustment

	22
	000-255
	Green 1 fine-tuning

	23
	000-255
	Blue 1 is a coarse adjustment

	24
	000-255
	Blue 1 fine-tuned

	25
	000-255
	White 1 coarse

	26
	000-255
	White 1 fine-tuned

	27
	000-255
	Y2 coarse adjustment (Y effect amplitude)

	28
	000-255
	Y2 fine-tuning 

	29
	000-255
	Zoom in 2

	30
	000-255
	Dimming 2 coarse adjustment

	31
	000-255
	Dimming 2 fine tuning

	32
	000-255
	Red 2 is a coarse adjustment

	33
	000-255
	Red 2 fine-tuned

	34
	000-255
	Green 2 is a coarse adjustment

	35
	000-255
	Green 2 fine-tuning

	36
	000-255
	Blue 2 is a coarse tone

	37
	000-255
	Blue 2 fine-tuned

	38
	000-255
	White 2 coarse

	39
	000-255
	White 2 fine-tuned

	40
	000-255
	Y3 coarse adjustment

	41
	000-255
	Y3 fine-tuning 

	42
	000-255
	Zoom in 3

	43
	000-255
	Dimming 3 coarse adjustment

	44
	000-255
	Dimming 3 fine tuning

	45
	000-255
	Red 3 is a coarse adjustment

	46
	000-255
	Red 3 fine-tuned

	47
	000-255
	Green 3 is a coarse adjustment

	48
	000-255
	Green 3 fine-tuning

	49
	000-255
	Blue 3 is a coarse adjustment

	50
	000-255
	Blue 3 fine-tuned

	51
	000-255
	White 3 is a coarse tone

	52
	000-255
	White 3 fine-tuned

	53
	000-255
	Y4 coarse adjustment

	54
	000-255
	Y4 fine-tuning 

	55
	000-255
	Zoom in 4

	56
	000-255
	Dimming 4 coarse adjustment

	57
	000-255
	Dimming 4 fine tuning

	58
	000-255
	Red 4 is a coarse adjustment

	59
	000-255
	Red 4 fine-tuned

	60
	000-255
	Green 4 is a coarse adjustment

	61
	000-255
	Green 4 fine-tuning

	62
	000-255
	Blue 4 is a coarse tone

	63
	000-255
	Blue 4 fine-tuned

	64
	000-255
	White 4 coarse

	65
	000-255
	White 4 fine-tuned

	66
	000-255
	Y5 coarse adjustment

	67
	000-255
	Y5 fine-tuning 

	68
	000-255
	Zoom in 5

	69
	000-255
	Dimming 5 coarse adjustment

	70
	000-255
	Dimming 5 fine tuning

	71
	000-255
	Red 5 is a coarse adjustment

	72
	000-255
	Red 5 fine-tuning

	73
	000-255
	Green 5 coarse adjustment

	74
	000-255
	Green 5 fine-tuning

	75
	000-255
	Blue 5 is a coarse adjustment

	76
	000-255
	Blue 5 fine-tuned

	77
	000-255
	White 5 coarse

	78
	000-255
	White 5 fine-tuned

	79
	000-255
	Y6 coarse adjustment

	80
	000-255
	Y6 fine-tuning 

	81
	000-255
	Zoom in 6

	82
	000-255
	Dimming 6 coarse adjustment

	83
	000-255
	Dimming 6 fine tuning

	84
	000-255
	Red 6 is a coarse adjustment

	85
	000-255
	Red 6 fine-tuned

	86
	000-255
	Green 6 is a coarse adjustment

	87
	000-255
	Green 6 fine-tuning

	88
	000-255
	Blue 6 is a coarse tone

	89
	000-255
	Blue 6 fine-tuned

	90
	000-255
	White 6 coarse

	91
	000-255
	The white 6 was fine-tuned

	92
	000-255
	Y7 coarse adjustment

	93
	000-255
	Y7 fine-tuning 

	94
	000-255
	Zoom in 7

	95
	000-255
	Dimming 7 coarse adjustment

	96
	000-255
	Dimming 7 fine tuning

	97
	000-255
	Red 7 is a coarse adjustment

	98
	000-255
	Red 7 fine-tuned

	99
	000-255
	Green 7 is a coarse adjustment

	100
	000-255
	Green 7 fine-tuning

	101
	000-255
	Blue 7 is a coarse adjustment

	102
	000-255
	Blue 7 fine-tuned

	103
	000-255
	White 7 is a coarse cut

	104
	000-255
	The white 7 is fine-tuned

	105
	000-255
	Y8 coarse adjustment

	106
	000-255
	Y8 fine-tuning 

	107
	000-255
	Zoom in 8

	108
	000-255
	Dimming 8 coarse adjustment

	109
	000-255
	Dimming 8 micro-adjustments

	110
	000-255
	Red 8 is a coarse adjustment

	111
	000-255
	Red 8 fine-tuned

	112
	000-255
	Green 8 coarse adjustment

	113
	000-255
	Green 8 fine-tuning

	114
	000-255
	Blue 8 is a coarse adjustment

	115
	000-255
	Blue 8 fine-tuned

	116
	000-255
	White 8 coarse

	117
	000-255
	White 8 fine-tuned

	118
	000-255
	Y9 coarse adjustment

	119
	000-255
	Y9 fine-tuning 

	120
	000-255
	Zoom in 9

	121
	000-255
	Dimming 9 coarse adjustment

	122
	000-255
	Dimming 9 fine tuning

	123
	000-255
	Red 9 is a coarse adjustment

	124
	000-255
	Red 9 fine-tuned

	125
	000-255
	Green 9 is a coarse adjustment

	126
	000-255
	Green 9 fine-tuning

	127
	000-255
	Blue 9 is a coarse adjustment

	128
	000-255
	Blue 9 fine-tuned

	129
	000-255
	White 9 is a coarse cut

	130
	000-255
	The white 9 was fine-tuned

	131
	000-255
	Y10 coarse adjustment

	132
	000-255
	Y10 fine-tuning 

	133
	000-255
	Zoom in 10

	134
	000-255
	Adjust the dimming 10 coarse

	135
	000-255
	Dimming 10 fine-tuning

	136
	000-255
	Red 10 coarse adjustment

	137
	000-255
	Red 10 fine-tuning

	138
	000-255
	Green 10 coarse adjustment

	139
	000-255
	Green 10 fine-tuning

	140
	000-255
	Blue 10 coarse adjustment

	141
	000-255
	Blue 10 fine-tuned

	142
	000-255
	White 10 coarse adjustment

	143
	000-255
	White 10 fine-tuned

	144
	000-255
	Y11 is fine-tuned

	145
	000-255
	Y11 fine-tuning 

	146
	000-255
	Zoom in 11

	147
	000-255
	Dimming 11 coarse adjustment

	148
	000-255
	Dimming 11 fine-tuning

	149
	000-255
	Red 11 is a coarse adjustment

	150
	000-255
	Red 11 fine-tuned

	151
	000-255
	Green 11 coarse adjustment

	152
	000-255
	Green 11 fine-tuned

	153
	000-255
	Blue 11 is a coarse adjustment

	154
	000-255
	Blue 11 fine-tuned

	155
	000-255
	White 11 coarse adjustment

	156
	000-255
	White 11 fine-tuned

	157
	000-255
	Y12 is fine-tuned

	158
	000-255
	Y12 fine-tuning 

	159
	000-255
	Zoom in 12

	160
	000-255
	Dimming 12 coarse adjustment

	161
	000-255
	Dimming 12 fine-tuning

	162
	000-255
	Red 12 is a coarse adjustment

	163
	000-255
	Red 12 fine-tuned

	164
	000-255
	Green 12 coarse adjustment

	165
	000-255
	Green 12 fine-tuning

	166
	000-255
	Blue 12 coarse adjustment

	167
	000-255
	Blue 12 fine-tuned

	168
	000-255
	White 12 coarse adjustment

	169
	000-255
	White 12 fine-tuned


Channel CH169B description:
	 channel 
	Channel values
	 basic function 

	1
	000-255
	Y1 is coarse-tuned

	2
	000-255
	Y1 fine-tuning 

	3
	000-255
	Zoom in 1

	4
	000-255
	Dimming 1 coarse adjustment

	5
	000-255
	Dimming 1 fine adjustment

	6
	000-255
	Strobe 1

	7
	000-255
	Red 1 is a coarse adjustment

	8
	000-255
	Red 1 fine-tuned

	9
	000-255
	Green 1 is a coarse adjustment

	10
	000-255
	Green 1 fine-tuning

	11
	000-255
	Blue 1 is a coarse adjustment

	12
	000-255
	Blue 1 fine-tuned

	13
	000-255
	White 1 coarse

	14
	000-255
	White 1 fine-tuned

	15
	000-255
	Y2 coarse adjustment

	16
	000-255
	Y2 fine-tuning 

	17
	000-255
	Zoom in 2

	18
	000-255
	Dimming 2 coarse adjustment

	19
	000-255
	Dimming 2 fine tuning

	20
	000-255
	Strobe 2

	21
	000-255
	Red 2 is a coarse adjustment

	22
	000-255
	Red 2 fine-tuned

	23
	000-255
	Green 2 is a coarse adjustment

	24
	000-255
	Green 2 fine-tuning

	25
	000-255
	Blue 2 is a coarse tone

	26
	000-255
	Blue 2 fine-tuned

	27
	000-255
	White 2 coarse

	28
	000-255
	White 2 fine-tuned

	29
	000-255
	Y3 coarse adjustment

	30
	000-255
	Y3 fine-tuning 

	31
	000-255
	Zoom in 3

	32
	000-255
	Dimming 3 coarse adjustment

	33
	000-255
	Dimming 3 fine tuning

	34
	000-255
	Strobe 3

	35
	000-255
	Red 3 is a coarse adjustment

	36
	000-255
	Red 3 fine-tuned

	37
	000-255
	Green 3 is a coarse adjustment

	38
	000-255
	Green 3 fine-tuning

	39
	000-255
	Blue 3 is a coarse adjustment

	40
	000-255
	Blue 3 fine-tuned

	41
	000-255
	White 3 is a coarse tone

	42
	000-255
	White 3 fine-tuned

	43
	000-255
	Y4 coarse adjustment

	44
	000-255
	Y4 fine-tuning 

	45
	000-255
	Zoom in 4

	46
	000-255
	Dimming 4 coarse adjustment

	47
	000-255
	Dimming 4 fine tuning

	48
	000-255
	Strobe 4

	49
	000-255
	Red 4 is a coarse adjustment

	50
	000-255
	Red 4 fine-tuned

	51
	000-255
	Green 4 is a coarse adjustment

	52
	000-255
	Green 4 fine-tuning

	53
	000-255
	Blue 4 is a coarse adjustment

	54
	000-255
	Blue 4 fine-tuned

	55
	000-255
	White 4 coarse

	56
	000-255
	White 4 fine-tuned

	57
	000-255
	Y5 coarse adjustment

	58
	000-255
	Y5 fine-tuning 

	59
	000-255
	Zoom in 5

	60
	000-255
	Dimming 5 coarse adjustment

	61
	000-255
	Dimming 5 fine tuning

	62
	000-255
	Strobe 5

	63
	000-255
	Red 5 is a coarse adjustment

	64
	000-255
	Red 5 fine-tuning

	65
	000-255
	Green 5 is a coarse adjustment

	66
	000-255
	Green 5 fine-tuning

	67
	000-255
	Blue 5 is a coarse adjustment

	68
	000-255
	Blue 5 fine-tuned

	69
	000-255
	White 5 coarse

	70
	000-255
	White 5 fine-tuned

	71
	000-255
	Y6 coarse adjustment

	72
	000-255
	Y6 fine-tuning 

	73
	000-255
	Zoom in 6

	74
	000-255
	Dimming 6 coarse adjustment

	75
	000-255
	Dimming 6 fine tuning

	76
	000-255
	Strobe 6

	77
	000-255
	Red 6 is a coarse adjustment

	78
	000-255
	Red 6 fine-tuned

	79
	000-255
	Green 6 is a coarse adjustment

	80
	000-255
	Green 6 fine-tuning

	81
	000-255
	Blue 6 is a coarse tone

	82
	000-255
	Blue 6 fine-tuned

	83
	000-255
	White 6 coarse

	84
	000-255
	The white 6 was fine-tuned

	85
	000-255
	Y7 coarse adjustment

	86
	000-255
	Y7 fine-tuning 

	87
	000-255
	Zoom in 7

	88
	000-255
	Dimming 7 coarse adjustment

	89
	000-255
	Dimming 7 fine tuning

	90
	000-255
	Strobe 7

	91
	000-255
	Red 7 is a coarse adjustment

	92
	000-255
	Red 7 fine-tuned

	93
	000-255
	Green 7 is a coarse adjustment

	94
	000-255
	Green 7 fine-tuning

	95
	000-255
	Blue 7 is a coarse adjustment

	96
	000-255
	Blue 7 fine-tuned

	97
	000-255
	White 7 is a coarse cut

	98
	000-255
	The white 7 was fine-tuned

	99
	000-255
	Y8 coarse adjustment

	100
	000-255
	Y8 fine-tuning 

	101
	000-255
	Zoom in 8

	102
	000-255
	Dimming 8 coarse adjustment

	103
	000-255
	Dimming 8 micro-adjustments

	104
	000-255
	Strobe 8

	105
	000-255
	Red 8 is a coarse adjustment

	106
	000-255
	Red 8 fine-tuned

	107
	000-255
	Green 8 coarse adjustment

	108
	000-255
	Green 8 fine-tuning

	109
	000-255
	Blue 8 is a coarse adjustment

	110
	000-255
	Blue 8 fine-tuned

	111
	000-255
	White 8 coarse

	112
	000-255
	White 8 fine-tuned

	113
	000-255
	Y9 coarse adjustment

	114
	000-255
	Y9 fine-tuning 

	115
	000-255
	Zoom in 9

	116
	000-255
	Dimming 9 coarse adjustment

	117
	000-255
	Dimming 9 fine tuning

	118
	000-255
	Strobe 9

	119
	000-255
	Red 9 is a coarse adjustment

	120
	000-255
	Red 9 fine-tuned

	121
	000-255
	Green 9 is a coarse adjustment

	122
	000-255
	Green 9 fine-tuning

	123
	000-255
	Blue 9 is a coarse adjustment

	124
	000-255
	Blue 9 fine-tuned

	125
	000-255
	White 9 is a coarse cut

	126
	000-255
	The white is fine-tuned to 9

	127
	000-255
	Y10 coarse adjustment

	128
	000-255
	Y10 fine-tuning 

	129
	000-255
	Zoom in 10

	130
	000-255
	Adjust the dimming 10 coarse

	131
	000-255
	Adjust the light 10 times

	132
	000-255
	Strobe 10

	133
	000-255
	Red 10 coarse adjustment

	134
	000-255
	Red 10 fine-tuning

	135
	000-255
	Green 10 coarse adjustment

	136
	000-255
	Green 10 fine-tuning

	137
	000-255
	Blue 10 coarse adjustment

	138
	000-255
	Blue 10 fine-tuned

	139
	000-255
	White 10 coarse adjustment

	140
	000-255
	White 10 fine-tuned

	141
	000-255
	Y11 is fine-tuned

	142
	000-255
	Y11 fine-tuning 

	143
	000-255
	Zoom in 11

	144
	000-255
	Dimming 11 coarse adjustment

	145
	000-255
	Dimming 11 fine tuning

	146
	000-255
	Strobe 11

	147
	000-255
	Red 11 is a coarse adjustment

	148
	000-255
	Red 11 fine-tuned

	149
	000-255
	Green 11 coarse adjustment

	150
	000-255
	Green 11 fine-tuned

	151
	000-255
	Blue 11 is a coarse adjustment

	152
	000-255
	Blue 11 fine-tuned

	153
	000-255
	White 11 coarse adjustment

	154
	000-255
	White 11 fine-tuned

	155
	000-255
	Y12 is fine-tuned

	156
	000-255
	Y12 fine-tuning 

	157
	000-255
	Zoom in 12

	158
	000-255
	Dimming 12 coarse adjustment

	159
	000-255
	Dimming 12 fine-tuning

	160
	000-255
	Strobe 12

	161
	000-255
	Red 12 is a coarse adjustment

	162
	000-255
	Red 12 fine-tuned

	163
	000-255
	Green 12 coarse adjustment

	164
	000-255
	Green 12 fine-tuning

	165
	000-255
	Blue 12 coarse adjustment

	166
	000-255
	Blue 12 fine-tuned

	167
	000-255
	White 12 coarse

	168
	000-255
	White 12 fine-tuned

	169
	000-255
	 function 


Channel CH101 description:
	 channel 
	Channel values
	 basic function 

	1
	000-255
	Y1 coarse adjustment (Y mode direction)

	2
	000-255
	Y1 fine-tuning 

	3
	000-255
	Y2 coarse adjustment (Y mode amplitude)

	4
	000-255
	Y2 fine-tuning 

	5
	000-255
	Y3 coarse adjustment

	6
	000-255
	Y3 fine-tuning 

	7
	000-255
	Y4 coarse adjustment

	8
	000-255
	Y4 fine-tuning 

	9
	000-255
	Y5 coarse adjustment

	10
	000-255
	Y5 fine-tuning 

	11
	000-255
	Y6 coarse adjustment

	12
	000-255
	Y6 fine-tuning 

	13
	000-255
	Y7 coarse adjustment

	14
	000-255
	Y7 fine-tuning 

	15
	000-255
	Y8 coarse adjustment

	16
	000-255
	Y8 fine-tuning 

	17
	000-255
	Y9 coarse adjustment

	18
	000-255
	Y9 fine-tuning 

	19
	000-255
	Y10 coarse adjustment

	20
	000-255
	Y10 fine-tuning 

	21
	000-255
	Y11 is fine-tuned

	22
	000-255
	Y11 fine-tuning 

	23
	000-255
	Y12 is fine-tuned

	24
	000-255
	Y12 fine-tuning 

	25
	000-255
	Y speed (Y effect speed)

	26
	000-255
	Y pattern 

	27
	000-255
	CTC

	28
	000-255
	Color macro

	29
	000-255
	 pattern 

	30
	000-255
	Built-in LED effects

	31
	000-255
	LED built-in effect speed

	32
	000-255
	LED built-in effect tail time

	33
	000-255
	LED background colour 

	34
	000-255
	Lightly adjust the LED background color tone

	35
	000-255
	 aiming 

	36
	000-255
	 stroboflash 

	37
	000-255
	Zoom in 1

	38
	000-255
	Zoom in 2

	39
	000-255
	Zoom in 3

	40
	000-255
	Zoom in 4

	41
	000-255
	Zoom in 5

	42
	000-255
	Zoom in 6

	43
	000-255
	Zoom in 7

	44
	000-255
	Zoom in 8

	45
	000-255
	Zoom in 9

	46
	000-255
	Zoom in 10

	47
	000-255
	Zoom in 11

	48
	000-255
	Zoom in 12

	49
	000-255
	 function 

	50
	000-255
	 red 

	51
	000-255
	 green 

	52
	000-255
	 blue 

	53
	000-255
	 white 

	54
	000-255
	Red 1

	55
	000-255
	Green 1

	56
	000-255
	Blue 1

	57
	000-255
	White 1

	58
	000-255
	Red 2

	59
	000-255
	Green 2

	60
	000-255
	Blue 2

	61
	000-255
	White 2

	62
	000-255
	Red 3

	63
	000-255
	Green 3

	64
	000-255
	Blue 3

	65
	000-255
	White 3

	66
	000-255
	Red 4

	67
	000-255
	Green 4

	68
	000-255
	Blue 4

	69
	000-255
	White 4

	70
	000-255
	Red 5

	71
	000-255
	Green 5

	72
	000-255
	Blue 5

	73
	000-255
	White 5

	74
	000-255
	Red 6

	75
	000-255
	Green 6

	76
	000-255
	Blue 6

	77
	000-255
	White 6

	78
	000-255
	Red 7

	79
	000-255
	Green 7

	80
	000-255
	Blue 7

	81
	000-255
	White 7

	82
	000-255
	Red 8

	83
	000-255
	Green 8

	84
	000-255
	Blue 8

	85
	000-255
	White 8

	86
	000-255
	Red 9

	87
	000-255
	Green 9

	88
	000-255
	Blue 9

	89
	000-255
	White 9

	90
	000-255
	Red 10

	91
	000-255
	Green 10

	92
	000-255
	Blue 10

	93
	000-255
	White 10

	94
	000-255
	Red 11

	95
	000-255
	Green 11

	96
	000-255
	Blue 11

	97
	000-255
	White 11

	98
	000-255
	Red 12

	99
	000-255
	Green 12

	100
	000-255
	Blue 12

	101
	000-255
	White 12


CH155 Channel Description:
	 channel 
	Channel values
	 basic function 

	1
	000-255
	Y1 coarse adjustment (Y mode direction)

	2
	000-255
	Y1 fine-tuning 

	3
	000-255
	Y2 coarse adjustment (Y mode amplitude)

	4
	000-255
	Y2 fine-tuning 

	5
	000-255
	Y3 coarse adjustment

	6
	000-255
	Y3 fine-tuning 

	7
	000-255
	Y4 fine-tuning

	8
	000-255
	Y4 fine-tuning 

	9
	000-255
	Y5 coarse adjustment

	10
	000-255
	Y5 fine-tuning 

	11
	000-255
	Y6 coarse adjustment

	12
	000-255
	Y6 fine-tuning 

	13
	000-255
	Y7 coarse adjustment

	14
	000-255
	Y7 fine-tuning 

	15
	000-255
	Y8 coarse adjustment

	16
	000-255
	Y8 fine-tuning 

	17
	000-255
	Y9 coarse adjustment

	18
	000-255
	Y9 fine-tuning 

	19
	000-255
	Y10 coarse adjustment

	20
	000-255
	Y10 fine-tuning 

	21
	000-255
	Y11 is fine-tuned

	22
	000-255
	Y11 fine-tuning 

	23
	000-255
	Y12 is fine-tuned

	24
	000-255
	Y12 fine-tuning 

	25
	000-255
	Y speed (Y mode speed)

	26
	000-255
	Y pattern 

	27
	000-255
	CTC

	28
	000-255
	Color macro

	29
	000-255
	 pattern 

	30
	000-255
	Built-in LED effects

	31
	000-255
	LED built-in effect speed

	32
	000-255
	LED built-in effect tail time

	33
	000-255
	LED background colour 

	34
	000-255
	Lightly adjust the LED background color tone

	35
	000-255
	LED background tone light fine tuning

	36
	000-255
	Adjust the dimming coarse

	37
	000-255
	Dimming fine-tuning

	38
	000-255
	 stroboflash 

	39
	000-255
	Zoom in 1

	40
	000-255
	Zoom in 2

	41
	000-255
	Zoom in 3

	42
	000-255
	Zoom in 4

	43
	000-255
	Zoom in 5

	44
	000-255
	Zoom in 6

	45
	000-255
	Zoom in 7

	46
	000-255
	Zoom in 8

	47
	000-255
	Zoom in 9

	48
	000-255
	Zoom in 10

	49
	000-255
	Zoom in 11

	50
	000-255
	Zoom in 12

	51
	000-255
	 function 

	52
	000-255
	Red undertones

	53
	000-255
	Red tweaks

	54
	000-255
	Greenish tinge

	55
	000-255
	Green tweaks

	56
	000-255
	Blue tinted

	57
	000-255
	Blue fine-tuning

	58
	000-255
	White undertones

	59
	000-255
	White fine-tuning

	60
	000-255
	Red 1 is a coarse adjustment

	61
	000-255
	Red 1 fine-tuning

	62
	000-255
	Green 1 coarse adjustment

	63
	000-255
	Green 1 fine-tuning

	64
	000-255
	Blue 1 is a coarse adjustment

	65
	000-255
	Blue 1 fine-tuned

	66
	000-255
	White 1 coarse

	67
	000-255
	White 1 fine-tuned

	68
	000-255
	Red 2 is a coarse adjustment

	69
	000-255
	Red 2 fine-tuned

	70
	000-255
	Green 2 is a coarse adjustment

	71
	000-255
	Green 2 fine-tuning

	72
	000-255
	Blue 2 is a coarse tone

	73
	000-255
	Blue 2 fine-tuned

	74
	000-255
	White 2 coarse

	75
	000-255
	White 2 fine-tuned

	76
	000-255
	Red 3 is a coarse adjustment

	77
	000-255
	Red 3 fine-tuned

	78
	000-255
	Green 3 is a coarse adjustment

	79
	000-255
	Green 3 fine-tuning

	80
	000-255
	Blue 3 is a coarse adjustment

	81
	000-255
	Blue 3 fine-tuned

	82
	000-255
	White 3 is a coarse tone

	83
	000-255
	White 3 fine-tuned

	84
	000-255
	Red 4 is a coarse adjustment

	85
	000-255
	Red 4 fine-tuned

	86
	000-255
	Green 4 is a coarse adjustment

	87
	000-255
	Green 4 fine-tuning

	88
	000-255
	Blue 4 is a coarse adjustment

	89
	000-255
	Blue 4 fine-tuned

	90
	000-255
	White 4 coarse

	91
	000-255
	White 4 fine-tuned

	92
	000-255
	Red 5 is a coarse adjustment

	93
	000-255
	Red 5 fine-tuned

	94
	000-255
	Green 5 coarse adjustment

	95
	000-255
	Green 5 fine-tuning

	96
	000-255
	Blue 5 is a coarse adjustment

	97
	000-255
	Blue 5 fine-tuned

	98
	000-255
	White 5 coarse

	99
	000-255
	White 5 fine-tuned

	100
	000-255
	Red 6 is a coarse adjustment

	101
	000-255
	Red 6 fine-tuned

	102
	000-255
	Green 6 is a coarse adjustment

	103
	000-255
	Green 6 fine-tuning

	104
	000-255
	Blue 6 is a coarse tone

	105
	000-255
	Blue 6 fine-tuned

	106
	000-255
	White 6 coarse

	107
	000-255
	The white 6 was fine-tuned

	108
	000-255
	Red 7 is a coarse adjustment

	109
	000-255
	Red 7 fine-tuned

	110
	000-255
	Green 7 coarse adjustment

	111
	000-255
	Green 7 fine-tuning

	112
	000-255
	Blue 7 is a coarse adjustment

	113
	000-255
	Blue 7 fine-tuned

	114
	000-255
	White 7 is a coarse cut

	115
	000-255
	The white 7 is fine-tuned

	116
	000-255
	Red 8 is a coarse adjustment

	117
	000-255
	Red 8 fine-tuned

	118
	000-255
	Green 8 coarse adjustment

	119
	000-255
	Green 8 fine-tuning

	120
	000-255
	Blue 8 is a coarse adjustment

	121
	000-255
	Blue 8 fine-tuned

	122
	000-255
	White 8 coarse

	123
	000-255
	White 8 fine-tuned

	124
	000-255
	Red 9 is a coarse adjustment

	125
	000-255
	Red 9 fine-tuned

	126
	000-255
	Green 9 is a coarse adjustment

	127
	000-255
	Green 9 fine-tuning

	128
	000-255
	Blue 9 is a coarse adjustment

	129
	000-255
	Blue 9 fine-tuned

	130
	000-255
	White 9 coarse

	131
	000-255
	The white 9 was fine-tuned

	132
	000-255
	Red 10 coarse adjustment

	133
	000-255
	Red 10 fine-tuning

	134
	000-255
	Green 10 coarse adjustment

	135
	000-255
	Green 10 fine-tuning

	136
	000-255
	Blue 10 coarse adjustment

	137
	000-255
	Blue 10 fine-tuned

	138
	000-255
	White 10 coarse adjustment

	139
	000-255
	White 10 fine-tuned

	140
	000-255
	Red 11 is a coarse adjustment

	141
	000-255
	Red 11 fine-tuned

	142
	000-255
	Green 11 coarse adjustment

	143
	000-255
	Green 11 fine-tuned

	144
	000-255
	Blue 11 is a coarse adjustment

	145
	000-255
	Blue 11 fine-tuned

	146
	000-255
	White 11 coarse adjustment

	147
	000-255
	White 11 fine-tuned

	148
	000-255
	Red 12 is a coarse adjustment

	149
	000-255
	Red 12 fine-tuned

	150
	000-255
	Green 12 coarse adjustment

	151
	000-255
	Green 12 fine-tuning

	152
	000-255
	Blue 12 coarse adjustment

	153
	000-255
	Blue 12 fine-tuned

	154
	000-255
	White 12 coarse adjustment

	155
	000-255
	White 12 fine-tuned


Channel CH179 description:
	 channel 
	Channel values
	 basic function 

	1
	000-255
	Y1 coarse adjustment (Y mode direction)

	2
	000-255
	Y1 fine-tuning 

	3
	000-255
	Y2 coarse adjustment (Y mode amplitude)

	4
	000-255
	Y2 fine-tuning 

	5
	000-255
	Y3 coarse adjustment

	6
	000-255
	Y3 fine-tuning 

	7
	000-255
	Y4 fine-tuning

	8
	000-255
	Y4 fine-tuning 

	9
	000-255
	Y5 coarse adjustment

	10
	000-255
	Y5 fine-tuning 

	11
	000-255
	Y6 coarse adjustment

	12
	000-255
	Y6 fine-tuning 

	13
	000-255
	Y7 coarse adjustment

	14
	000-255
	Y7 fine-tuning 

	15
	000-255
	Y8 coarse adjustment

	16
	000-255
	Y8 fine-tuning 

	17
	000-255
	Y9 coarse adjustment

	18
	000-255
	Y9 fine-tuning 

	19
	000-255
	Y10 coarse adjustment

	20
	000-255
	Y10 fine-tuning 

	21
	000-255
	Y11 is fine-tuned

	22
	000-255
	Y11 fine-tuning 

	23
	000-255
	Y12 is fine-tuned

	24
	000-255
	Y12 fine-tuning 

	25
	000-255
	Y speed (Y mode speed)

	26
	000-255
	Y pattern 

	27
	000-255
	CTC

	28
	000-255
	Color macro

	29
	000-255
	 pattern 

	30
	000-255
	Built-in LED effects

	31
	000-255
	LED built-in effect speed

	32
	000-255
	LED built-in effect tail time

	33
	000-255
	LED background colour 

	34
	000-255
	Lightly adjust the LED background color tone

	35
	000-255
	LED background tone light fine tuning

	36
	000-255
	Adjust the dimming coarse

	37
	000-255
	Dimming fine-tuning

	38
	000-255
	 stroboflash 

	39
	000-255
	Zoom in 1

	40
	000-255
	Zoom in 2

	41
	000-255
	Zoom in 3

	42
	000-255
	Zoom in 4

	43
	000-255
	Zoom in 5

	44
	000-255
	Zoom in 6

	45
	000-255
	Zoom in 7

	46
	000-255
	Zoom in 8

	47
	000-255
	Zoom in 9

	48
	000-255
	Zoom in 10

	49
	000-255
	Zoom in 11

	50
	000-255
	Zoom in 12

	51
	000-255
	 function 

	52
	000-255
	Red undertones

	53
	000-255
	Red tweaks

	54
	000-255
	Greenish tinge

	55
	000-255
	Green tweaks

	56
	000-255
	Blue tinted

	57
	000-255
	Blue fine-tuning

	58
	000-255
	White undertones

	59
	000-255
	White fine-tuning

	60
	000-255
	Dimming 1 coarse adjustment

	61
	000-255
	Dimming 1 fine adjustment

	62
	000-255
	Red 1 is coarse

	63
	000-255
	Red 1 fine-tuning

	64
	000-255
	Green 1 coarse adjustment

	65
	000-255
	Green 1 fine-tuning

	66
	000-255
	Blue 1 is a coarse adjustment

	67
	000-255
	Blue 1 fine-tuned

	68
	000-255
	White 1 coarse

	69
	000-255
	White 1 fine-tuned

	70
	000-255
	Dimming 2 coarse adjustment

	71
	000-255
	Dimming 2 fine tuning

	72
	000-255
	Red 2 is a coarse adjustment

	73
	000-255
	Red 2 fine-tuned

	74
	000-255
	Green 2 is a coarse adjustment

	75
	000-255
	Green 2 fine-tuning

	76
	000-255
	Blue 2 is a coarse tone

	77
	000-255
	Blue 2 fine-tuned

	78
	000-255
	White 2 coarse

	79
	000-255
	White 2 fine-tuned

	80
	000-255
	Dimming 3 coarse adjustment

	81
	000-255
	Dimming 3 fine tuning

	82
	000-255
	Red 3 is a coarse adjustment

	83
	000-255
	Red 3 fine-tuned

	84
	000-255
	Green 3 is a coarse adjustment

	85
	000-255
	Green 3 fine-tuning

	86
	000-255
	Blue 3 is a coarse adjustment

	87
	000-255
	Blue 3 fine-tuned

	88
	000-255
	White 3 is a coarse tone

	89
	000-255
	White 3 fine-tuned

	90
	000-255
	Dimming 4 coarse adjustment

	91
	000-255
	Dimming 4 fine tuning

	92
	000-255
	Red 4 is a coarse adjustment

	93
	000-255
	Red 4 fine-tuned

	94
	000-255
	Green 4 is a coarse adjustment

	95
	000-255
	Green 4 fine-tuning

	96
	000-255
	Blue 4 is a coarse tone

	97
	000-255
	Blue 4 fine-tuned

	98
	000-255
	White 4 coarse

	99
	000-255
	White 4 fine-tuned

	100
	000-255
	Dimming 5 coarse adjustment

	101
	000-255
	Dimming 5 fine tuning

	102
	000-255
	Red 5 is a coarse adjustment

	103
	000-255
	Red 5 fine-tuning

	104
	000-255
	Green 5 is a coarse adjustment

	105
	000-255
	Green 5 fine-tuning

	106
	000-255
	Blue 5 is a coarse adjustment

	107
	000-255
	Blue 5 fine-tuned

	108
	000-255
	White 5 coarse

	109
	000-255
	White 5 fine-tuned

	110
	000-255
	Dimming 6 coarse adjustment

	111
	000-255
	Dimming 6 fine tuning

	112
	000-255
	Red 6 is a coarse adjustment

	113
	000-255
	Red 6 fine-tuned

	114
	000-255
	Green 6 is a coarse adjustment

	115
	000-255
	Green 6 fine-tuning

	116
	000-255
	Blue 6 is a coarse tone

	117
	000-255
	Blue 6 fine-tuned

	118
	000-255
	White 6 coarse

	119
	000-255
	The white 6 was fine-tuned

	120
	000-255
	Dimming 7 coarse adjustment

	121
	000-255
	Dimming 7 fine tuning

	122
	000-255
	Red 7 is a coarse adjustment

	123
	000-255
	Red 7 fine-tuned

	124
	000-255
	Green 7 is a coarse adjustment

	125
	000-255
	Green 7 fine-tuning

	126
	000-255
	Blue 7 is a coarse adjustment

	127
	000-255
	Blue 7 fine-tuned

	128
	000-255
	White 7 is a coarse cut

	129
	000-255
	The white 7 is fine-tuned

	130
	000-255
	Dimming 8 coarse adjustment

	131
	000-255
	Dimming 8 micro-adjustments

	132
	000-255
	Red 8 is a coarse adjustment

	133
	000-255
	Red 8 fine-tuned

	134
	000-255
	Green 8 coarse adjustment

	135
	000-255
	Green 8 fine-tuning

	136
	000-255
	Blue 8 is a coarse adjustment

	137
	000-255
	Blue 8 fine-tuned

	138
	000-255
	White 8 coarse

	139
	000-255
	White 8 fine-tuned

	140
	000-255
	Dimming 9 coarse adjustment

	141
	000-255
	Dimming 9 fine tuning

	142
	000-255
	Red 9 is a coarse adjustment

	143
	000-255
	Red 9 fine-tuned

	144
	000-255
	Green 9 is a coarse adjustment

	145
	000-255
	Green 9 fine-tuning

	146
	000-255
	Blue 9 is a coarse adjustment

	147
	000-255
	Blue 9 fine-tuned

	148
	000-255
	White 9 is a coarse cut

	149
	000-255
	The white 9 was fine-tuned

	150
	000-255
	Adjust the dimming 10 coarse

	151
	000-255
	Dimming 10 fine-tuning

	152
	000-255
	Red 10 coarse adjustment

	153
	000-255
	Red 10 fine-tuning

	154
	000-255
	Green 10 coarse adjustment

	155
	000-255
	Green 10 fine-tuning

	156
	000-255
	Blue 10 coarse adjustment

	157
	000-255
	Blue 10 fine-tuned

	158
	000-255
	White 10 coarse adjustment

	159
	000-255
	White 10 fine-tuned

	160
	000-255
	Dimming 11 coarse adjustment

	161
	000-255
	Dimming 11 fine-tuning

	162
	000-255
	Red 11 is a coarse adjustment

	163
	000-255
	Red 11 fine-tuned

	164
	000-255
	Green 11 coarse adjustment

	165
	000-255
	Green 11 fine-tuned

	166
	000-255
	Blue 11 is a coarse adjustment

	167
	000-255
	Blue 11 fine-tuned

	168
	000-255
	White 11 coarse adjustment

	169
	000-255
	White 11 fine-tuned

	170
	000-255
	Dimming 12 coarse adjustment

	171
	000-255
	Dimming 12 fine-tuning

	172
	000-255
	Red 12 is a coarse adjustment

	173
	000-255
	Red 12 fine-tuned

	174
	000-255
	Green 12 coarse adjustment

	175
	000-255
	Green 12 fine-tuning

	176
	000-255
	Blue 12 coarse adjustment

	177
	000-255
	Blue 12 fine-tuned

	178
	000-255
	White 12 coarse

	179
	000-255
	White 12 fine-tuned


[image: image2.jpg]Color Chart

Value _|Percent/Setting
000 |No function
001 & 002 |White 2700K R =156 G=118 B=0 w=63
003 & 004 |White 3200K R =156 G=141 B=5 w =89
005 & 006 |White 4200K R =156 G=141 B=14 W =255
007 & 008 |White 5600K R =156 G =207 B=54 W =255
009 & 010 |White 8000K R =130 G=255 B=96 W =255
011 [Blue R=0 G=0 B =255 w=0
012 ¢ 048 |+ Green R=0 G=0-255 B =255 w=0
049 [Cyan R=0 G=255 B =255 w=0
050 < 086 |- Blue R=0 G=255 B=255-0 w=0
087 [Green R=0 G=255 B=0 w=0
088 & 124 [+ Red R=0-255 G=255 B=0 w=0
125 |Yellow R=255 G=255 B=0 w=0
126 & 162 |- Green R=255 G=255-0 B=0 w=0
163 |Red R=255 G=0 B=0 w=0
164 & 200 |+ Blue R=255 G=0 B=0-255 w=0
201 |Magenta R=255 G=0 B =255 w=0
202 % 238 |- Red R=255-0 G=0 B=255 w=0
239 [Blue R=0 G=0 B =255 w=0
240 247 [Color fade, fast to slow
248 ¢ 255 [Color snap, fast to slow




[image: image3.jpg]Strobe Settings

Value _|Percent/Setting || value |PercentiSetting
000 & 019 [OFf 145 149 [On
020 & 024 (On 150 & 164 [Random strobe 0-100%, fast to slow
025 ¢ 064 [Strobe, fast to slow 165 169 [On
065 & 069 (On 170 & 184 [Puse strobe, fast to slow
070 % 084 [Strobe 100-0%, fast to slow 185 189 [On
085 & 089 (On 190 & 204 |Random pulse strobe, fast to slow
090 ¢ 104 [Strobe 0-100%, fast to slow 205 ¢ 209 (On
105 & 109 (On 210 & 224 [Strobe 0-100-0%, fast to slow
110 ¢ 124 [Random strobe, fast to slow 225 229 (On
125 & 129 |On 230 & 244 |Random pulse strobe, fast to slow
130 & 144 [Random strobe 100-0%, fasttoslow || 245 ¢ 255 [On
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V. Technical parameters:
Voltage: AC100~240V 50/60HZ
Power: 12*60W (800W)
Lighting beads: 12 four-in-one 60 watt LED lighting beads
Control mode: DMX512, self-walking, master and slave, sound control, with RDM function.
Channel: CH20.CH169A.CH169B.CH53.CH101.CH155.CH179
Dimming: 32bit linear dimming from 0 to 100%
Features: single swing + staining + beam
Working temperature: -30 ~50 degrees
Flicker frequency: 1~30HZ
Appearance: metal, black
Connection mode: DMX512 input/output / power input/output.
IP class: IP20
Size: Weight:                                Size: Weight:
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