200WCOB strobe + pixel background
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Read the instructions before use
 technical parameter ：
Voltage: AC90-240V,50/60Hz
Power: 220W
Light source: 216pcs 0.2W SMD5050 RGB 3IN1 LED LED+200WCOB
Control channel: 17/160 CH two channel modes
Control mode: DMX512, master and slave, self-walking, sound control
Connection: XLR IN + OUT, PowerCon IN + OUT
IP protection level: IP20
Exterior material: flame retardant engineering plastic
It has high speed blackout/flash function, circle control, rich and gorgeous color pixels and other effects
Product size: 485*295*260
Net weight: 5.2kg
1. Panel operation:
	Addr（ address ）
	d(001-512)

	STAT（ static state ）
	RED（ red ）
	D (0-255)

	
	Gren（ hispid arthraxon ）
	

	
	Blue（ blue ）
	

	
	White (white)
	

	
	STRB（ stroboflash ）
	

	AUTO (self-driving)
	Au.01 (self-walk 1)
	S (01-9) self-walking speed

	
	Au.02 (self-walk 2)
	

	
	…
	

	
	Au.14 (self-walk 14)
	

	
	Au.15 (self-walk 15)
	

	Soud（ sound control ）
	Sod1 (sonar 1)
	SC- (1-9) Voice control sensitivity

	
	Sod2 (sonar 2)
	

	CH（ pattern ）
	Channel 17 (17-channel mode)

	
	CH160 (160-channel mode)

	DISP (Screen Inversion Settings)
	Display the reverse setting


Channel table
	Channel 17 mode
	 function 
	DMX price 
	 description 

	1
	General dimming
	0-255
	0-100%

	2
	 stroboflash 
	0-19
	 inaction 

	
	
	20-255
	The strobe goes from slow to fast

	3
	 white 
	0-255
	0-100%

	4
	Positive red
	0-255
	0-100%

	5
	Positive green
	0-255
	0-100%

	6
	Positive blue
	0-255
	0-100%

	7
	Positive background color
	0-10
	 inaction 

	
	
	11-255
	 background colour 

	8
	The positive background color is dimmed in total
	0-255
	0-100%

	9
	Positive scenario
	0-10
	 inaction 

	
	
	11-15
	Scenario 1

	
	
	16-20
	Scenario 2

	
	
	21-25
	Scenario 3

	
	
	26-30
	Scenario 4

	
	
	31-35
	Scenario 5

	
	
	36-40
	Scenario 6

	
	
	41-45
	Scenario 7

	
	
	46-50
	Scenario 8

	
	
	51-55
	Scenario 9

	
	
	56-60
	Scenario 10

	
	
	61-65
	Scenario 11

	
	
	66-70
	Scenario 12

	
	
	71-75
	Scenario 13

	
	
	76-80
	Scenario 14

	
	
	81-85
	Scenario 15

	
	
	86-90
	Scenario 16

	
	
	91-95
	Scenario 17

	
	
	96-100
	Scenario 18

	
	
	101-105
	Scenario 19

	
	
	106-110
	Scenario 20

	
	
	111-115
	Scenario 21

	
	
	116-120
	Scenario 22

	
	
	121-125
	Scenario 23

	
	
	126-130
	Scenario 24

	
	
	131-135
	Scenario 25

	
	
	136-140
	Scenario 26

	
	
	141-145
	Scenario 27

	
	
	146-150
	Scenario 28

	
	
	151-155
	Scenario 29

	
	
	156-160
	Scenario 30

	
	
	161-165
	Scenario 31

	
	
	166-170
	Scenario 32

	
	
	171-175
	Scenario 33

	
	
	176-180
	Scenario 34

	
	
	181-185
	Scenario 35

	
	
	186-190
	Scenario 36

	
	
	191-195
	Scenario 37

	
	
	196-200
	Scenario 38

	
	
	201-205
	Scenario 39

	
	
	206-210
	Scenario 40

	
	
	211-215
	Scenario 41

	
	
	216-220
	Scenario 42

	
	
	221-225
	Scenario 43

	
	
	226-230
	Scenario 44

	
	
	231-235
	Scenario 45

	
	
	236-245
	Voice control 1

	
	
	246-255
	Voice-activated 2

	10
	Positive scenario speed
	0-255
	The scene speed is from slow to fast

	11
	Reverse red
	0-255
	0-100%

	12
	Reverse green
	0-255
	0-100%

	13
	Reverse blue
	0-255
	0-100%

	14
	Reverse background color
	0-10
	 inaction 

	
	
	11-255
	 background colour 

	15
	Reverse background color is always dimmed
	0-255
	0-100%

	16
	Reverse scenario
	0-10
	 inaction 

	
	
	11-15
	Scenario 1

	
	
	16-20
	Scenario 2

	
	
	21-25
	Scenario 3

	
	
	26-30
	Scenario 4

	
	
	31-35
	Scenario 5

	
	
	36-40
	Scenario 6

	
	
	41-45
	Scenario 7

	
	
	46-50
	Scenario 8

	
	
	51-55
	Scenario 9

	
	
	56-60
	Scenario 10

	
	
	61-65
	Scenario 11

	
	
	66-70
	Scenario 12

	
	
	71-75
	Scenario 13

	
	
	76-80
	Scenario 14

	
	
	81-85
	Scenario 15

	
	
	86-90
	Scenario 16

	
	
	91-95
	Scenario 17

	
	
	96-100
	Scenario 18

	
	
	101-105
	Scenario 19

	
	
	106-110
	Scenario 20

	
	
	111-115
	Scenario 21

	
	
	116-120
	Scenario 22

	
	
	121-125
	Scenario 23

	
	
	126-130
	Scenario 24

	
	
	131-135
	Scenario 25

	
	
	136-140
	Scenario 26

	
	
	141-145
	Scenario 27

	
	
	146-150
	Scenario 28

	
	
	151-155
	Scenario 29

	
	
	156-160
	Scenario 30

	
	
	161-165
	Scenario 31

	
	
	166-170
	Scenario 32

	
	
	171-175
	Scenario 33

	
	
	176-180
	Scenario 34

	
	
	181-185
	Scenario 35

	
	
	186-190
	Scenario 36

	
	
	191-195
	Scenario 37

	
	
	196-200
	Scenario 38

	
	
	201-205
	Scenario 39

	
	
	206-210
	Scenario 40

	
	
	211-215
	Scenario 41

	
	
	216-220
	Scenario 42

	
	
	221-225
	Scenario 43

	
	
	226-230
	Scenario 44

	
	
	231-235
	Scenario 45

	
	
	236-245
	Voice control 1

	
	
	246-255
	Voice-activated 2

	17
	Reverse scene speed
	0-255
	The scene speed is from slow to fast

	
	
	
	

	
	
	
	

	160 channel mode
	 function 
	DMX price 
	 description 

	1
	 white light 
	0-255
	0-100%

	2
	Red 1
	0-255
	0-100%

	3
	Green 1
	0-255
	0-100%

	4
	Blue 1
	0-255
	0-100%

	5
	Red 2
	0-255
	0-100%

	6
	Green 2
	0-255
	0-100%

	7
	Blue 2
	0-255
	0-100%

	8
	Red 3
	0-255
	0-100%

	9
	Green 3
	0-255
	0-100%

	10
	Blue 3
	0-255
	0-100%

	11
	Red 4
	0-255
	0-100%

	12
	Green 4
	0-255
	0-100%

	13
	Blue 4
	0-255
	0-100%

	14
	Red 5
	0-255
	0-100%

	15
	Green 5
	0-255
	0-100%

	16
	Blue 5
	0-255
	0-100%

	：
	
	
	


