800W Cutting Light Instruction  manual                                      800W Cutting Light Instruction  manual   [image: ]                                          




800W Cutting Moving Head Pattern Light
Instruction manual
(RDM, color display, touch operation)
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PLEASE READ THIS CAREFULLY BEFORE USE

source

AC100-240V, 50/60Hz

Power consumption: 900W

light source

800W LED module

LED Lifespan: 20000 hours  
 
Color temperature:8700K

effect

Zoom angle: 4.8°-50 °

Fixed Colors: 6 preset colors + white + effects 

CMY Mixing System: Independent CMY color mixing channels
 
Color Temperature Adjustment: CTO 2500K-6500K (linear adjustment)

Frequency: Up to 25Hz                Modes: Random strobe, Pulse strobe

control

Signal Interface: 3-pin XLR/ 5-pin XLR (optional)

Control Protocols: DMX512, RDM

Channel Modes: 35CH
Operating Modes: Auto-run, Master/Slave synchronization

IP level :IP20 

N. W: 28.5 KG                     G.W: 33 KG






























































































Channel table


	Channel 1
	Function
	DMX Value
	Description

	[ CH1 ]
	X Shaft
	0-255
	0-540 degrees

	[ CH2 ]
	X-axis fine adjustment
	0-255
	0-2 degrees

	[ CH3 ]
	Y Shaft
	0-255
	0-270 degrees

	[ CH4 ]
	Y-axis fine adjustment
	0-255
	0-1 degree

	[ CH5 ]
	XY Velocity
	0-255
	Horizontal/vertical speed from fast to slow

	[ CH6]
	Strobe
	0-3
	Turn off the light

	
	
	4-103
	Pulse strobe from slow to fast

	
	
	104-107
	Switch

	
	
	108-207
	Gradient strobe from slow to fast

	
	
	208-212
	Switch

	
	
	213-251
	Random strobe from slow to fast

	
	
	252-255
	Switch

	[ CH7]
	Dimming
	0-255
	0-100% dimming

	[ CH8]
	cyan
	0-255
	

	[ CH9]
	magenta
	0-255
	

	[ CH10]
	Yellow
	0-255
	

	[ CH11]
	Temperature
	0-255
	

	[ CH12]
	Color wheel
	 0-4
	white light

	
	
	 5-9
	White light color + Color 1

	
	
	 10-14
	Color 1

	
	
	 15-19
	Color 1 + Color 2

	
	
	 20-24
	Color 2

	
	
	 25-29
	Color 2 + Color 3

	
	
	 30-34
	Color3

	
	
	 35-39
	Color 3 + Color 4

	
	
	 40-44
	Color 4

	
	
	 45-49
	Color 4 + Color 5






	[ CH12]
	Color disc
	 50-54
	Color 5

	
	
	 55-59
	Color 5 + Color 6

	
	
	 60-64
	Color 6

	
	
	 65-255
	Reverse flow from slow to fast

	[ CH13]
	Ra
	 0-127
	/

	
	
	 128-255
	Insert the Ra

	[ CH14 ]
	Gobo wheel
	 0-9
	white light

	
	
	 10-19
	Pattern 1

	
	
	 20-29
	Pattern 2

	
	
	 30-39
	Pattern 3

	
	
	 40-49
	Pattern 4

	
	
	 50-59
	Pattern 5

	
	
	 60-69
	Pattern 6

	
	
	 70-79
	Jitter pattern from slow to fast 1

	
	
	 80-89
	Jitter pattern from slow to fast 2

	
	
	 90-99
	Jitter pattern from slow to fast 3

	
	
	 100-109
	Jitter pattern from slow to fast 4

	
	
	 110-119
	Jitter pattern from slow to fast 5

	
	
	 120-129
	Jitter pattern from slow to fast 6

	
	
	 130-191
	Reverse flow from  fast to slow

	
	
	 192-255
	Positive flow from slow to fast

	[ CH15 ]
	Rotating gobo wheel
	 0-9
	white light

	
	
	 10-19
	Pattern 1

	
	
	 20-29
	Pattern 2

	
	
	 30-39
	Pattern 3

	
	
	 40-49
	Pattern 4

	
	
	 50-59
	Pattern 5

	
	
	 60-69
	Pattern 6






	[ CH15 ]
	Rotating gobo wheel
	 70-79
	Pattern 7

	
	
	 80-89
	Jitter pattern from slow to fast 1

	
	
	 90-99
	Jitter pattern from slow to fast 2

	
	
	 100-109
	Jitter pattern from slow to fast 3

	
	
	 110-119
	Jitter pattern from slow to fast 4

	
	
	 120-129
	Jitter pattern from slow to fast 5

	
	
	 130-139
	Jitter pattern from slow to fast 6

	
	
	 140-149
	Jitter pattern from slow to fast 7

	
	
	 150-190
	Reverse flow from  fast to slow

	
	
	 191-192
	Stop

	
	
	 193-255
	Positive flow from slow to fast

	[ CH16 ]
	Gobo wheel rotates automatic-ally
	 0-127
	0-360 degrees

	
	
	 128-190
	Reverse flow from  fast to slow

	
	
	 191-192
	Stop

	
	
	 193-255
	Positive flow from slow to fast

	[ CH17 ]
	Gobo wheel effect
	 0-255
	

	[ CH18 ]
	Zoom
	 0-255
	From big to small

	[ CH19 ]
	Focusing
	 0-255
	From far to near

	[ CH20 ]
	Focus fine-tuning
	 0-255
	

	[ CH21 ]
	Prism 1
	 0-127
	/

	
	
	 128-255
	

	[ CH22 ]
	Prism rotates automatic-ally
	 0-127
	0-360 degrees

	
	
	 128-187
	Positive flow from fast to slow

	
	
	 188-195
	Stop

	
	
	 196-255
	Reverse flow from  slow to fast

	[ CH23 ]
	Atomization  1
	 0-3
	/

	
	
	 4-255
	Linear atomization





	 [ CH24 ]
	Slice 1
	 0-255
	

	 [ CH25 ]
	Slice 2
	 0-255
	

	 [ CH26 ]
	Slice 3
	 0-255
	

	 [ CH27 ]
	Slice 4
	 0-255
	

	 [ CH28 ]
	Slice 5
	 0-255
	

	 [ CH29 ]
	Slice 6
	 0-255
	

	 [ CH30 ]
	Slice 7
	 0-255
	

	 [ CH31 ]
	Slice 8
	 0-255
	

	 [ CH32 ]
	Slice rotation
	 0-255
	

	 [ CH33 ]
	Aperture
	 0-255
	

	 [ CH34 ]
	Slice macro
	0-7
	/

	
	
	8-135
	Twenty-eight patterns

	
	
	136-255
	Pattern switching from slow to fast

	 [ CH35 ]
	Reset
/Function
	 0-209
	Non-functional

	
	
	 210-215
	Reset the XY motor after 3 seconds

	
	
	 216-219
	Non-functional

	
	
	 220-235
	Reset the effect motor after 3 seconds

	
	
	 236-239
	Non-functional

	
	
	 240-255
	Reset the whole light after 3 seconds
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